InS_StArT
EN2000.COM
1.0
^Compex EN2000N Ethernet Adapter,EN2000.COM,IE0
!OIE0 (CABLE) Cable Type
?Select the cable type.
BNC
TPI
!OIE0 (PORT) I/O Base Port
?The driver will automatically read the I/O Base Port of your adapter if this entry is unspecified.
240
280
2C0
300
320
340
360
!OIE0 (INT) Hardware Interrupt
?The driver will automatically read the Interrupt Level of your adapter if this entry is unspecified.
2
3
4
5
10
11
!OIE0 (NODE ADDRESS) Optional Node Address
0
7FFFFFFFFFFF
*RIE0 (FRAME) Frame Types
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
!OIE0 (ADAPTERNUM) Adapter Number
?Specify the adapter you wish to initialize if you have multiple adapters installed.
1
2
3
4
5
6
7
8
InS_EnD
