InS_StArT
RL100A.COM
1.0
^Compex RL100ATX PCI Fast Ethernet Adapter,RL100A.COM,IE0
?This driver supports only PCI machine
$OIE0(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFFF
*RIE0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers. 
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
!OIE0(LINESPEED)Line Speed
?NOTE: The line speed will be autodetected on driver's load.
10M
100M
@AUTODETECT
!OIE0(FULLDUPLEX)Full Duplex Function
?NOTE: The full duplex function will be autodetected on driver's load.
DISABLE
ENABLE
@AUTODETECT
InS_EnD

 
