InS_StArT
RLPNPA.COM
2.20
^Compex RL2000A PnP Series Ethernet Card,RLPNPA.COM,IE0
!OIE0 (PORT) I/O Base Port
?The driver will automatically read the I/O Base Port of your adapter if this entry is unspecified.
220
240
260
280
2A0
2C0
2E0
300
320
340
360
380
3A0
3C0
3E0
!OIE0 (INT) Hardware Interrupt
?The driver will automatically read the Interrupt Level of your adapter if this entry is unspecified.
3
4
5
9
10
11
12
15
!OIE0 (NODE ADDRESS) Optional Node Address
0
7FFFFFFFFFFF
*RIE0 (FRAME) Frame Types
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
!OIE0 (BOARD) Board Number
?Specify the adapter you wish to initialize if you have multiple adapters installed.
1
2
3
4
InS_EnD
