Model Name: ADSL-USB (For Conexant Chipset) Version: 02 Table of Contents: FCC Part 68 FCC Part 15 Chapter 1 Introduction Chapter 2 Determine your connection settings Chapter 3 Install the driver and make a connection Chapter 3.1 Windows 98/98SE Chapter 3.1.1 Setting the ADSL VPI & VCI For RFC 1483/2364/2516 Chapter 3.1.2 Making a RFC 1483 connection - Win98/98SE Chapter 3.1.3 Making a RFC 2364/2516 connection - Win98/98SE Chapter 3.2 Windows 2000 Chapter 3.2.1 Setting the ADSL VPI & VCI For RFC 1483/2364/2516 Chapter 3.2.2 Making a RFC 1483 connection - Win2000 Chapter 3.2.3 Making a RFC 2364/2516 connection - Win2000 Chapter 3.3 Windows Me Chapter 3.3.1 Setting the ADSL VPI & VCI For RFC 1483/2364/2516 Chapter 3.3.2 Marking a RFC 1483 Connection - WinMe Chapter 3.3.3 Making a RFC 2364/2516 Connection - WinMe Chapter 3.4 Windows XP (Home Edition) Chapter 3.4.1 Setting the ADSL VPI & VCI For RFC 1483/2364/2516 Chapter 3.4.2 Marking a RFC 1483 Connection - WinXP Chapter 3.4.3 Making a RFC 2364/2516 Connection - WinXP Declaration of CE Declaration of conformity to type FCC Part 68 This equipment complies with Part 68 of the FCC Rules. On the bottom of this equipment is a label that contains the FCC Registration Number and Ringer Equivalence Number (REN) for this equipment. You must provide this information to the telephone company upon request. The REN is useful to determine the quantity of devices you may connect to the telephone line and still have all of those devices ring when your number is called. In most, but not all areas, the sum of the REN of all devices connected to one line should not exceed five (5.0). To be certain of the number of devices you may connect to your line, as determined by the REN, you should contact your local telephone company to determine the maximum REN for your calling area. If the modem causes harm to the telephone network, the telephone company may discontinue your service temporarily. If possible, they will notify you in advance. But if advance notice isn't practical, you will be notified as soon as possible. You will be advised of your right to file a complaint with the FCC. The telephone company may make changes in its facilities, equipment, operations, or procedures that could affect the proper operation of your equipment. If they do, you will be notified in advance to give you an opportunity to maintain uninterrupted telephone service. If you experience trouble with this modem, please contact your dealer for repair/warranty information. The telephone company may ask you to disconnect this equipment from the network until the problem has been corrected or you are sure that the equipment is not malfunctioning. This equipment may not be used on coin service provided by the telephone company. Connection to party lines is subject to state tariffs. Installation This device is equipped with a USOC RJ11C connector. Table of Contents FCC Part 15 The modem generates and uses radio frequency energy. If it is not installed and used properly in strict accordance with the user's manual, it may cause interference with radio and television reception. The modem has been tested and found to comply with the limits for Class B computing devices in accordance with the specifications in Subpart B, Part 15 of the FCC regulations. These specifications are designed to provide reasonable protection against such interference in a residential installation. However, there is no guarantee that interference will not occur in a particular installation. FCC regulations require that shielded interface cables be used with your modem. If interference does occur, we suggest the following measures be taken to rectify the problem: 1) Move the receiving antenna. 2) Move the modem away from the radio or TV. 3) Plug the modem into a different electrical outlet. 4) Discuss the problem with a qualified radio/TV technician. CAUTION : Changes or modifications not expressly approved by the party responsible for compliance to the FCC Rules could void the user's authority to operate this equipment. Cable connections: All equipment connected to this modem must use shielded cable as the interconnection means. Notes: Operation is subject to the following two conditions: (1) This device may not cause harmful interference, and (2) This device must accept any interference received including interference that may cause undesired operation. Chapter 1 Introduction Introduction This driver supports the Conexant USB ADSL reference board. This release contains both LAN (RFC 1483) and WAN (RFC 2364/RFC 2516). Supported Operating Systems - Windows 98 - Windows 2000 - Windows Me - Windows XP Supported ATM Protocols - PPP over ATM VCMUX (RFC 2364) (WAN) - PPP over ATM LLC (RFC 2364) (WAN) - PPP over Ethernet (PPPoE) LLC SNAP (RFC 2516) (WAN) - PPP over Ethernet (PPPoE) VCMUX (RFC 2516) (WAN) - Bridged IP over ATM LLCSNAP (RFC 1483) (LAN) - Routed IP over ATM LLCSNAP (RFC 1483) (LAN) - Bridged IP over ATM VCMUX (RFC 1483) (LAN) - Routed IP over ATM VCMUX (RFC 1483) (LAN) - Classic IP over ATM (RFC1577) LED Interface
RXD illuminated when data is received from the ADSL line.
HS illuminated when data is transmitted to the ADSL line.
LNK illuminated when the ADSL transceiver is in Showtime Mode.
RDY illuminated when the device is successfully enumerated on the USB.
Chapter 2 Determine your connection settings You need to know your PC systems Windows OS and Internet Protocol supplied by your ADSL service provider. Refer to the following chart for your ADSL Driver. Protocol Selection RFC1483 -> Bridged Ethernet over ATM RFC2364 -> Point-to-Point Protocol over ATM RFC2516 -> Point-to-Point Protocol over Ethernet
ADSL Driver Selection | Directory (Win98/98SE/2000/Me/XP)
RFC1483 -> Bridged Ethernet over ATM | CD-ROM:\ Driver\LAN
RFC2364 -> Point-to-Point Protocol over ATM | CD-ROM:\ Driver\WAN
RFC2516 -> Point-to-Point Protocol over Ethernet | CD-ROM:\ Driver\WAN
Having determined the ADSL Driver you will be installing, you now need to gather the connection information supplied by your ADSL service provider. VPI value: VCI value: Framing: VC / MUX LLC / SNAP Mode: ANSI T1.413 ITU G.lite ITU G.dmt
For RFC1483 | For RFC2364 or 2516
Host: | User Name:
Domain: | Password:
Gateway: | Host or IP Address:
IP Address: |
Subnet Mask: |
DNS or server address: |
Chapter 3 Install the driver and make a connection You will be installing drivers and then proceeding to make an Internet connection. This process requires you to enter in information as prompted by the Microsoft Installation Wizard. <Note> You may need the Microsoft Windows Operating System installation files (CAB files) to complete the installation. The CAB files are contained in the Microsoft's system CD-ROM. Some systems may have already installed the CAB files to the hard drive, but you should have the Microsoft Windows CD-ROM handy just in case. Proceed now to the installation procedure for the Windows Operating System installed in your computer. Windows 98/98SE Windows 2000 Windows Me Windows XP 3.1 Windows 98 / 98SE <Step01> Insert the USB Plug into the USB port of ADSL USB. The Add New Hardware Wizard window will automatically appear to indicate that a new USB Network Controller has been found. Click Next. <Step02> Still in the Add New Hardware Wizard. You will be asked "What do you want Windows to do?" Select the Search for the best driver for your device option, then click Next. <Step03> Insert the ADSL Driver CD into your systems CD-ROM drive, Select Driver Directory LAN or WAN, Then click Next. If you need to set for RFC 1483 to select LAN subdirectory and for RFC 2516/2364 to select WAN subdirectory. <Step04> The Add New Hardware Wizard will appear and indicate the Conexant AccessRunner USB ADSL Interface has been recognized and will install a new driver. Click Next. <Step05> At the conclusion of the ADSL modem driver installation, the Add New Hardware Wizard window appears and displays your new installed Conexant AccessRunner USB ADSL Interface. Click Finish. 3.1.1 Setting the ADSL VPI & VCI For RFC 1483/2364/2516 <Step01> Double click the "Conexant AccessRunner" Icon in Control Panel or on the desktop. - You can use Alt-P or Alt-C to make sure or change VPI / VCI. - Make sure the VPI & VCI without problem. <Step02> This is the Network Protocol and PVC settings section. Enter in the VPI & VCI and Framing values supplied by your ADSL service provider. Press "Apply". When you install LAN mode, you can select several modes from "Ecapsulation mode", such as "Bridged IP over ATM LLC SNAP (RFC1483)", "Routed IP over ATM LLC SNAP (RFC1483)", "Bridged IP over ATM VCMUX (RFC1483)" or "Routed IP over ATM VCMUX (RFC1483)". When you install WAN mode, you can select several modes from "Ecapsulation mode", such as "PPP over ATM VCMUX (RFC2364)", "PPP over ATM LLC SNAP (RFC 2364)", "PPP over Ethernet LLC SNAP (RFC 2516)" or "PPP over Ethernet VCMUX (RFC 2516)". Chapter 3.1.2 Making a RFC 1483 connection - Win98/98SE <Step01> From the Start menu on the tool bar, select Settings, Control Panel and then double-click on the Network icon. The Network window appears. Select the Configuration tab, scroll the installed network component window and find Conexant AccessRunner USB ADSL LAN Adapter. <Step02> Scroll the installed network component window and select TCP/IP -> Conexant AccessRunner USB ADSL LAN Adapter. Then click the Properties button. The TCP/IP Properties window will appear. Select the IP Address tab and then select the Specify an IP Address option. Enter the IP Address and Subnet Mask settings supplied by your ADSL provider. <Step03> To setup a new gateway, select the Gateway tab, and then enter the setting in the New Gateway section. Click Add. Select DNS Configuration tab. <Step04> Select the Enable DNS option. - Enter your host name into Host: box. - Enter your domain name into Domain: box. - Enter DNS number into DNS Server Search Order box and click Add. If you have more than one DNS numbers, repeat this step. - After setting all the necessary TCP/IP properties, click OK. <Step05> The Network window appears. Click OK. Chapter 3.1.3 Making a RFC 2364/2516 connection - Win98/98SE After installation, you will find AccessRunner DSL shortcut on the desktop. You can use it to dial out and make a connection with your ISP. <Step01> Click the Access Runner DSL on the desktop and enter the User Name and Password supplied by your Internet service provider (ISP). Then click Connect. <Step02> The Connection Established window appear. Inernet service is now established. Click Close and then the Diagnostic tool icon will appear on the task bar. Chapter 3.2 Windows 2000 Insert USB plug into USB port of ADSL modem. <Step01> After inserting, the Found New Hardware Wizard will appear. Click Next. <Step02> Still in the Found New Hardware Wizard, select the Search for a suitable device... option. Click Next. <Step03> Next you will be prompted for software drivers. Select specify a location. <Step04> Insert the ADSL Driver CD into your systems CD-ROM drive, Select Driver Directory LAN or WAN,Then click OK. If you need to set for RFC 1483 to select LAN subdirectory and for RFC 2516/2364 to select WAN sub directory. <Step05> The Found New Hardware Wizard will then find the ADSL USB MODEM, click Next. <Step06> The Digital Signature Not Found window appears. You will be asked; Do you want to continue installation? Click Yes. <Step07> The Found New Hardware Wizard will prompt that Windows has finished installing the software for this device, then Click Finish. Chapter 3.2.1 Setting the ADSL VPI & VCI For RFC 1483/2364/2516 <Step01> Double click the "Conexant AccessRunner" Icon in Control Panel or on desktop. - You can use Alt-P or Alt-C to make sure or change VPI / VCI. - Make sure the VPI & VCI without problem. <Step02> This is the Network Protocol and PVC settings section. Enter in the VPI & VCI and Framing values supplied by your ADSL service provider. Press "Apply". When you install LAN mode, you can select several modes from "Ecapsulation mode", such as "Bridged IP over ATM LLC SNAP (RFC1483)", "Routed IP over ATM LLC SNAP (RFC1483)", "Bridged IP over ATM VCMUX (RFC1483)" or "Routed IP over ATM VCMUX (RFC1483)". When you install WAN mode, you can select several modes from "Ecapsulation mode", such as "PPP over ATM VCMUX (RFC2364)", "PPP over ATM LLC SNAP (RFC 2364)", "PPP over Ethernet LLC SNAP (RFC 2516)" or "PPP over Ethernet VCMUX (RFC 2516)". Chapter 3.2.2 Making a RFC 1483 connection - Win2000 <Step01> Double-click My Computer, Control Panel and then Network and Dial-up Connection, The Network and Dial-up Connections window appears. Right-click on the Local Area Connection, and then click on properties. <Step02> The Local Area Connection window appears. Click on Internet Protocol (TCP/IP), then click on Properties. <Step03> The Internet Protocol (TCP/IP) window appears. Under the General tab, enable Use the following IP address. The default settings for IP configurations will turn from gray to clear. Enter in the IP address, Subnet Mask, and Default Gateway supplied by your ADSL service provider. Click OK. <Step04> The previous General Tab window appears. Click OK. Chapter 3.2.3 Making a RFC 2364/2516 connection - Win2000 After installation, you will find AccessRunner DSL shortcut on the desktop. You can use it to dial out and make a connection with your ISP. <Step01> The Connect My Connection window will appear. Enter your User Name and Password supplied by your ADSL service provider. You are now ready to make a network connection, Click Dial. <Step02> The Connection complete window appears, click OK. Chapter 3.3 Windows Me Insert the USB plug into the USB port of ADSL modem. <Step01> The Add New Hardware Wizard window will automatically appear to indicate that a new ADSL USB MODEM has been found. Select the Specify the location of the driver option. Click Next. <Step02> Insert the ADSL Driver CD into your systems CD-ROM drive, Select Driver Directory LAN or WAN,Then click Next. If you need to set for RFC 1483 to select LAN subdirectory and for RFC 2516/2364 to select WAN sub directory. <Step03> The Add New Hardware Wizard will appear and indicate the Conexant AccessRunner USB ADSL Interface has been recognized and will install a new driver. Click Next. <Step04> At the conclusion of the ADSL modem driver installation, the Add New Hardware Wizard window appears and displays your newly installed Conexant AccessRunner USB ADSL Interface, then click Finish. Chapter 3.3.1 Setting the ADSL VPI & VCI For RFC 1483/2364/2516 <Step01> Double click the "Conexant AccessRunner" Icon in Control Panel. - You can use Alt-P or Alt-C to make sure or change VPI / VCI. - Make sure the VPI & VCI without problem. <Step02> This is the Network Protocol and PVC settings section. Enter in the VPI & VCI and Framing values supplied by your ADSL service provider. Press "Apply". When you install LAN mode, you can select several modes from "Ecapsulation mode", such as "Bridged IP over ATM LLC SNAP (RFC1483)", "Routed IP over ATM LLC SNAP (RFC1483)", "Bridged IP over ATM VCMUX (RFC1483)" or "Routed IP over ATM VCMUX (RFC1483)". When you install WAN mode, you can select several modes from "Ecapsulation mode", such as "PPP over ATM VCMUX (RFC2364)", "PPP over ATM LLC SNAP (RFC 2364)", "PPP over Ethernet LLC SNAP (RFC 2516)" or "PPP over Ethernet VCMUX (RFC 2516)". Chapter 3.3.2 Marking a RFC 1483 Connection - WinMe <Step01> From the Start menu on the tool bar, select Settings, Control Panel and then double-click on the Network icon. The Network window appears. Select the Configuration tab, scroll the installed network component window and find Conexant AccessRunner USB ADSL LAN Adapter. <Step02> Scroll the installed network component window and select TCP/IP -> Conexant AccessRunner USB ADSL LAN Adapter. Then click the Properties button. The TCP/IP Properties window will appear. Select the IP Address tab and then select the Specify an IP Address option. Enter the IP Address and Subnet Mask settings supplied by your ADSL provider. <Step03> To setup a new gateway, select the Gateway tab, and then enter the setting in the New Gateway section. Click Add. Select DNS Configuration tab. <Step04> Select the Enable DNS option. - Enter your host name into Host: box. - Enter your domain name into Domain: box. - Enter DNS number into DNS Server Search Order box and click Add. If you have more than one DNS numbers, repeat this step. - After setting all the necessary TCP/IP properties, click OK. <Step05> The Network window appears, Click OK. Chapter 3.3.3 Making a RFC 2364/2516 Connection - WinMe After installation, you will find AccessRunner DSL shortcut on the desktop. You can use it to dial out and make a connection with your ISP. <Step01> The Connect To window appears. Enter the User Name and Password supplied by your Internet service provider (ISP). Then click Connect. <Step02> The Connection Established window appear. Internet service is now established. Click Close and then the Diagnostic tool icon will appear on the task bar. Chapter 3.4 Windows XP (Home Edition) Insert USB plug into the USB port of ADSL modem.. <Step01> The Add New Hardware Wizard window will automatically appear to indicate that a new ADSL USB Modem has been found. Select the Specify the location of the driver option. Click Next. <Step02> Insert the ADSL Driver CD into your systems CD-ROM drive, Select Driver Directory LAN or WAN,Then click Next. If you need to set for RFC 1483 to select LAN subdirectory and for RFC 2516/2364 to select WAN sub directory. If you Red ever been setup driver, you should select. <Step03> At the conclusion of the ADSL modem driver installation, the Add New Hardware Wizard window appears and displays your newly installed Conexant AccessRunner USB ADSL Interface, then click Finish. Chapter 3.4.1 Setting the ADSL VPI & VCI For RFC 1483/2364/2516 <Step01> Double click the "Conexant AccessRunner" Icon in Control Panel or on the desktop. - You can use Alt-P or Alt-C to make sure or change VPI / VCI. - Make sure the VPI & VCI without problem. <Step02> This is the Network Protocol and PVC settings section. Enter in the VPI & VCI and Framing values supplied by your ADSL service provider. Press "Apply". When you install LAN mode, you can select several modes from "Ecapsulation mode", such as "Bridged IP over ATM LLC SNAP (RFC1483)", "Routed IP over ATM LLC SNAP (RFC1483)", "Bridged IP over ATM VCMUX (RFC1483)" or "Routed IP over ATM VCMUX (RFC1483)". When you install WAN mode, you can select several modes from "Ecapsulation mode", such as "PPP over ATM VCMUX (RFC2364)", "PPP over ATM LLC SNAP (RFC 2364)", "PPP over Ethernet LLC SNAP (RFC 2516)" or "PPP over Ethernet VCMUX (RFC 2516)". Chapter 3.4.2 Marking a RFC 1483 Connection - WinXP (Home Edition) <Step01> From the Start menu on the tool bar, select Control Panel and then double-click on the Network connection icon. The Network connection window appears.Scroll installed network component window and find Conexant AccessRunner USB ADSL LAN Adapter, Click right key and select properties. <Step02> Scroll the installed network component window and select TCP/IP. Then click the Properties button. The TCP/IP Properties window will appear. Select the IP Address tab and then select the Specify an IP Address option. Enter the IP Address, Subnet Mask, default gateway and DNS server settings supplied by your ADSL provider. <Step03> The Network window appears. Click OK. Chapter 3.4.3 Making a RFC 2364/2516 Connection - WinXP (Home Edition) After installation, you will find AccessRunner DSL shortcut on the desktop. You can use it to dial out and make a connection with your ISP. <Step01> The Connect To window appears. Enter the User Name and Password supplied by your Internet service provider (ISP). Then click Connect. <Step02> The Connection Established window appear. Internet service is now established. Click Close and then the Diagnostic tool icon will appear on the task bar. Declaration of CE This declaration of conformity is according to article 7(3) and article 10(2) of the Council of European Communities of 3 May 1989. The protection requirements according the Council Directive article 4 and Annex III are kept. MODEL / TYPE: ADSL-USB This declaration is given from the manufacturer submitted by TRAINING RESEARCH CO., LTD. 5F,. NO. 571, SEC. 7, CHUNG HSIAO E. RD., TAIPEI, TAIWAN, R. O. C. To the judgement of the products with regard to electromagnetic compatibility according following regulations: EN 55022 Class B EN 50082 - 1 (IEC 801 Part 2,4 / ENV 50140 / ENV 50141) EN 60950 Declaration of conformity to type I hereby declare that the product MODEL/TYPE: ADSL-USB and satisfies all the technical regulations applicable to the product within the scope of Council Directives 91/263/EEC and 93/97/EEC: TBR21 The equipment has been approved to [Commission Decision No. 98/34/EG] for Pan-European single terminal connection to the Public Switched Telephone Network (PSTN). However, due to differences between the individual PSTNs provided in different countries the approval does not, of itself, give an unconditional assurance of successful operation on every PSTN network termination point. In the event of problems, you should contact your equipment supplier in the first instance. Part No.:506-10106-02