




                               ADSL - USB                                    
--------------------------------------------------------------------------------------
                             Quick Start Guide

Hardware Installation:
* Insert CD into the CD-ROM drive under Windows System.
* Install the USB Plug in the USB Port.
* Plug in the phone line to phone jack.
* Refer to the User's Manual for detailed setup procedure.
* The system found new hardware and would install the drivers for it.

There are LEDs for ADSL-USB useful information:
* RXD  illuminated when data is received from the ADSL line.
* HS   illuminated when data is transmitted to the ADSL line.
* LNK  illuminated when the ADSL transceiver is in Showtime Mode.
* RDY  illuminated when the device is successfully enumerated on the USB.
  
Software installation:
Driver for all major operating systems(Windows 98/2000/Me/XP).
For more detailed information, please refer to user's manual in Drivers CD.

Browse the Driver & Manual CD:
CD-ROM:\ Driver\ LAN\ subdirectory contains Bridged Ethernet over ATM (RFC1483).
CD-ROM:\ Driver\ WAN\ subdirectory contains Point-to-Point Protocol over ATM(RFC2364) 
                                        and Point-to-Point Protocol over Ethernet (RFC2516).
CD-ROM:\ Manual\ Manual.htm  user's manual by HTML format.
(Recommand to use IE3.0 later or Netscape 3.0 later to browse manual)





