InS_StArT
RETH.COM
1.0
^Ethernet MLID v3.04,RETH.COM,I00
!OI00(INT)Optional Hardware Interrupt
2
3
4
5
10
11
12
15
!OI00(PORT)Optional Base I/O Port
200
220
240
260
280
2C0
300
320
340
360
$OI00(NODE ADDRESS)Optional Node Address
?NOTE: Avoid any multicast address and broadcast address.
0
FFFFFFFFFFFF
*OI00(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
