SiS191/190 10/100/1000Mbs adapter manufacture test tools package release note

======
v2.02
======
1. Initial release.

======
v2.03
======
1. Modify the naming of executive file to indicate it is used for SiS191/190 
   only. ex. lan19x.exe
2. Add the needed file "MODERN.FON" while executing exlb19x.exe. 
3. Fix the issue fail to run Diag.exe.  

======
v2.04
======
1. DIAG19x.exe: Fix the problem of internal loopback test fail that happened 
   after external loopback test in half duplex mode. 

======
v2.05
======
1. DIAG19x.exe: Rx got packet when external loopback test failed in half duplex mode. 
2. DIAG19x.exe: Fix the issue that internal loopback test fails sometimes.

======
v2.06
======
1. DIAG19x.exe: Fix 2 station test package lose issue.

======
v2.09
======
1. DIAG19x.exe: Fix the issue that Node ID cannot be read.
2. DIAG19x.exe: Fix the issue of Tx error for Diag19x 100/Full internal loopback test.
3. DIAG19x.exe: Fix the issue of failure for MII and PCI registers test.
4. DIAG19x.exe: It is ready for Broadcom AC131 and Marvell 88e1111 PHY.

======
v2.10
======
1. Realtek RTL8211 PHY is supported.
2. Add 1000 Mbps external loopback test for RTL8211 PHY.

======
v2.11
======
1. Fix the issue that exlb19x can't set font.

======
v2.12
======
1. ee19x.exe can support 190/191 EEPROM signature auto recognization.

======
v2.13
======
1. Fix the halt issue on SiS656 & SiS649.

======
v2.14
======
1. Support SiS191 REV.01 on SiS966.
2. Support Marvell PHY new chip (PHY ID: 0x01410cc2)
3. Support RGMII mode.

======
v2.15
======
1. Fix the failuration of Agere MII register test. 

======
v2.16
======
1. Fix the conflict between PCI register test and USB Legacy support.

======
v2.17
======
1. Fix that setting Magic packet to power into S5 can not wake up

======
v2.18
======
1. Fix the wrong message will show when testing external loopback

======
v2.19
======
1. Support Attansic Phy F1

======
v2.20
======
1. Fix the link change wakeup event problem

======
v2.21
======
1. Solve RGMII will be set when south bridge is 996L but device is sis190

======
v2.22
======
1. Solve packet lost with Attansic phy.


======
v2.23
======
1. Workaround for AUSU motherboard (966+10M/100M PHY)
2. Detected cable is connect or not on Lan19x  and exlb19x

======
v2.24
======
1. Solve that the result will be pass if cable is unpluged during testing.

======
v2.25
======
1. Modify MII test for Realtek PHY RTL8021 (Offest 0x05, bit 10 & bit 11)

======
v2.26
======
1. Update ee19x to v1.01, but Diag19x, lan19x and exlb19x are still in v2.25

======
v2.27
======
1. Workaround for 968, and Diag19x, lan19x and exlb19x are in v2.27 for consistence of version
 
======
v2.28
======
1. Solve Media Tyape will show "Cable disconnect" and Auto Config will show "Cable disconnect"

======
v2.29
======
1. HW workaround

======
v2.30
======
1. Workaround for PHY RTL8211B

======
v2.31
======
1. Produce Lantest.log when excute lan19x.exe and exlb19x.exe
2. Update EE19x to v1.03 

======
v2.32
======
1. Solve that Regtest is failed in sis968 when load mac from eeprom