            SiS PCI Fast Ethernet Adapter Installation
              for Windows Millennium Edition Driver
            ==========================================

driver file:  .\sisnic.sys
INF file:     .\netoem.inf

Install The Driver
------------------

1.  Install the card in the PCI slot and connect the cable to the network;
    turn on the computer and start Windows ME. **HAVE YOUR WINDOWS ME CD
    ROM AVAILABLE** because you will need to copy some additional system
    files.

2.  When Windows ME starts, a "Add New Hardware Wizard" dialog box appears
    identifying the card as a "PCI Ethernet Controller".

    NOTE, if the "Add New Hardware Wizard" dialog box does not appear,
    please do the followings

    a. After entering Windows ME, double click "My Computer".
    b. Double click "Control Panel".
    c. Double click "System".
    d. Click the "Device Manager" tab.
    e. Open "Other Devices" (with a yellow "?" icon).
    f. Select "PCI Ethernet Controller" then click "Remove" button to
       remove it.

       Note, if you do not see any "PCI Ethernet Controller", Windows ME
       fails to detect your adapter. There may be problem with the adapter
       itself or with the system BIOS.

    g. Click Refresh and a "Add New Hardware Wizard" appears identifying
       the card as a "PCI Ethernet Controller";
    h. goto next step.

3.  Click Next then select "Search for the best driver for your device
    [Recommended]".

4.  Click Next then enable the "Specify a location" check box; specify the
    correct path in which SiS 900 PCI Fast Ethernet Adapter driver for WinME
    resides.

5.  Click Next then Windows ME identifies the card as
    "SiS 900 PCI Fast Ethernet Adapter"

6.  Click Finish to let Windows ME finishes the driver installation.


Adapter Configuration
---------------------

1. Double click "My Computer".
2. Double click "Control Panel".
3. Double click "Network" icon.
4. Select
   "SiS 900 PCI Fast Ethernet Adapter"
   then click "Properties..." button.
5. Click "Advanced" tab.
6. Here, you can set the following properties:

   <1>. MediaType

             100BaseTX
             100BaseTX Full_Duplex
             10BaseT Full_Duplex
             10BaseT
             AUTO_CONFIG   ;Default value if not set

   <2>. NetworkAddress

             Override the adapter's Ethernet address. Legal values are
             xx-xx-xx-xx-xx-xx, where xx is a hexadecimal byte value.
             Unless necessary, do NOT modify this field and let the
             system use the default Ethernet address contained in the
             serial ROM on the adapter.

   The following is supported for AMD LFPC project with SVID/SSID:1022/0900

   <3>. PhoneLineMediaType

             HighPowerHighSpeed
             HighPowerLowSpeed
             LowPowerHighSpeed
             LowPowerLowSpeed

   <4>. PhysicalLayer

             AUTO
             LAN
             HOME

        Note:
           1). When user select LAN or HOME item, the driver will
               force the connector to coresponding media (LAN or HOME).
           2). When user select AUTO item, the driver will auto-detect:
               a). if LAN is link-on, the driver will choice the connector
                   to LAN (Ethernet).
               b). otherwise, the driver will choice the connector to
                   HOME (Phone Line).

7. After setting the properties, you must restart your computer to
   make the changes effective.

---End of File---


