
               SiS 900/7016 PCI Fast Ethernet Adapter Installation 
                              for NDIS 2.0 Driver

(1) OS/2 installation instructions.

    1. On OS/2 desktop, double-click "OS/2 system" icon.
    2. Double-click "System setup" icon.
    3. Double-click "MPTS" icon.
    4. Click "OK" to enter MPTS.
    5. Select "Configure".
    6. Select "LAN adapter & protocol" and click "configure".
    7. Click "Other Adapters".
    8. Be sure that "SiS PCI Fast Ethernet Aapter Drivers" is in your computer.
       And specifies correct path. Ex: E:\NDIS2\OS2 (if driver in CD-ROM drive E)
    9. In "Network Adapters" menu, Select "SiS 900/7016 PCI Fast Ethernet
       Adapter".
    10. Add protocols you need.
    11. Click "OK"
    12. Click "Close"
    13. Click "Exit"
    14. System will update CONFIG.SYS for you. Click "Exit".
    15. Click "OK"
    16. Click "EXIT" to quit MPTS.
    17. Restart your computer.
 

(2) Optional Parameters
-----------------------

    SLOT           - This parameter specifies the slot number used for
                     notifications. For PCI slot, you can specify from
                     1 to 16.

    MEDIATYPE      - This parameter specifies the media type currently used.
                     If MEDIATYPE does not specified, it will auto detect the
                     media type.

                     Parameters List:
                       AUTO       -- Auto-select media type.
                       UTP        -- 10BaseT half duplex mode.
                       UTPFULL    -- 10BaseT full duplex mode.
                       FAST       -- 100BaseT half duplex mode.
                       FASTFULL   -- 100BaseT full duplex mode.

