******************************926sco5.txt************************************
*                                                                           *
*                         PCI Ethernet Adapter                              *
*                                                                           *
*                      Ethernet Driver for SCOUNIX 5.0                      *
*                                                                           *
*                         V.1.0,   Jan. 1998                                *
*                                                                           *
*****************************************************************************
                 
         
Introduction:
=============

    Below are instructions for creating an SCO "custom" installation diskette
containing the MDI device driver for Fast Ethernet network adapter family.
MDI drivers are used with SCO's Open Server 5.0 Operating System.  Once the
diskette is created, follow the SCO instructions for using the "custom" and
"netconfig" utilities to install the driver.


Contents of the Subdirectory:
=============================

    926sco5.a              The SCOUNIX 5.0 driver installation package in ASCII encoded format.
    926sco5.txt            This file.


Installation:
=============

   To begin, place the viavtcmdi.a file on a DOS formatted diskette.  926sco5.a is
an ASCII encoded, compressed, SCO UNIX diskette image file.  Place the
diskette in drive A on a computer with SCO UNIX installed.  If you wish to
use drive B, adjust the instructions below appropriately.

Now enter the following commands at the UNIX prompt.  Remember, UNIX is
case sensitive.

   doscp a:926sco5.a 926sco5.a  (copies from DOS disk to current working
                               directory)
   uudecode 926sco5.a         (decodes the ASCII file to binary VOL.000.000)

Now place the 3.5" diskette you want to become the installation diskette
in drive A.  This should be a UNIX formatted, high density diskette.
Enter the following command.  Again, if you wish to use drive B, adjust the
instructions below appropriately.

   dd if=VOL.000.000 of=/dev/rfd0135ds18 (transfers disk image to diskette)

The diskette is now ready to use with the SCO "custom" utility.
    
     After custom installation,use "netconfig" utility to set protocal for the card.



Note:
   926 PCI Ethernet Adapter has jumpless mode .You can use setup program to 
set card in jumpless mode .If your card is in jumpless mode,you must input correct
iobase during installing it.



