*****************************************************************************
*                                                                           *
*                         PCI Ethernet Adapter                              *
*                                                                           *
*               32 Bit ODI Driver for Client32 in DOS/Windows 3.x           *
*                                                                           *
*                         V. 3.63,   Jan. 1997                              *
*                                                                           *
*****************************************************************************

Introduction:
=============

  This document shows you how to setup the driver and how to use the enhanced
  functions by setting the custom keywords.


Contents of the Subdirectory:
=============================

    PCINWSRV.LAN        The 32 Bit ODI driver for Client32 in DOS/Windows 3.x.
    PCINWSRV.LDI        The installation information file.
    CNT32DOS.TXT        This file.


Installation:
=============

  Before starting with the installation process, make sure that the adapter
  is properly installed and configured. You can use the diagnostic program
  (A:\SETUP.EXE) in DOS mode to make sure your connection with the network is
  correct.

  Install Driver While setting up your Client32:
  ----------------------------------------------
    While you are installing Client32 programs, please have this driver
    diskette of the adapter near you.
    1. When the Installation program ask you to specify a lan driver, please
       select "OTHER DRIVERS" or "User Supplied Driver" to install driver from
       the diskette that come with your lan adapter.

    2. Insert the driver diskette into your floppy drive, and specify the
       path of the driver in the diskette(i.e. A:\NETWARE\CLIENT32.DOS) to copy
       the driver files to your system.

    3. A STARTNET.BAT file will be generated in the Client32 directory.
       (\NOVELL\CLIENT32 or other if you change the default path)

    4. When all the Clinet32 programs installation is completed, reboot your PC.


  System with existing Netware client programs:
  ---------------------------------------------
    If there are Client32 programs installed in your system already, you can
    use the following procedures to setup your driver.
    1. Add a Load driver command line to your STARTNET.BAT file in your
       Client32 directory. For example:

                LOAD C:\NOVELL\CLIENT32\PCINWSRV.LAN FRAME=Ethernet_802.2


       The following is a sample of the STARTNET.BAT file:

                SET NWLANGUAGE=ENGLISH
                C:\NOVELL\CLIENT32\NIOS.EXE
                LOAD C:\NOVELL\CLIENT32\LSLC32.NLM
                LOAD C:\NOVELL\CLIENT32\CMSM.NLM
                LOAD C:\NOVELL\CLIENT32\ETHERTSM.NLM
                LOAD C:\NOVELL\CLIENT32\PCINWSRV.LAN FRAME=Ethernet_802.2
                LOAD C:\NOVELL\CLIENT32\PCINWSRV.LAN FRAME=Ethernet_802.3
                LOAD C:\NOVELL\CLIENT32\IPX.NLM
                LOAD C:\NOVELL\CLIENT32\CLIENT32.NLM


    2. Execute STARTNET.BAT to connect to Server.


  NOTE:
  -----
    Multiple Lan Adapters in a system:
      If you want to install mutiple lan adapters in a server, you have to use
      the keyword, PCIID, to let driver locate the right adapter. You can use
      the diagnostic program (A:\SETUP.EXE) in DOS mode to show all the Ethernet
      addresses of your adapters. For example:

        LOAD PCINWSRV PCIID=00406300201A FRAME=Ethernet_802.2 NAME=Lan_1
        LOAD PCINWSRV PCIID=00406300201B FRAME=Ethernet_802.2 NAME=Lan_2



Configuration Parameters:
=========================
    Configuration:
    --------------
      You can the LOAD PCINWSRV.LAN command line parameters to configure the
      driver. There are special designed functions with this adapter which can
      accerate the performance. To enable the functions, for example:

        LOAD C:\NOVELL\CLIENT32\PCINWSRV.LAN FRAME=Ethernet_802.2 EAELYRECEIVE


    Custom Paremeters:
    ------------------
        EARLYTRANSMIT                   This keyword is used to enable turbo
                                        transmission mode for accelerating data
                                        transmission.

        EARLYRECEIVE                    This keyword is used to enable turbo
                                        receiption mode for accelerating data
                                        receiption.

        FULLDUPLEX                      This keyword is used to enable full
                                        duplex mode.

        PCIID = hhhhhhhhhhhh            This property is the Ethernet Address of
                                        the adapter you want to drive. If there
                                        are more than one ethernet adapters in
                                        your system, you have to use this
                                        property to let driver locate the right
                                        adapter. However, you don't have to use
                                        this property or let the value to be
                                        zero (i.e. PCIID = 0) if there is only
                                        one adapter in your system.

