*****************************************************************************
*                                                                           *
*                            PCI Ethernet Adapter                           *
*                                                                           *
*                  NDIS2 Driver for Lan Server DOS Workstations             *
*                                                                           *
*                            V. 2.91,   Jan. 1997                           *
*                                                                           *
*****************************************************************************

Introduction:
=============

  The Ethernet NDIS2 Driver for Lan Requester DOS workstations confirms to the
  Network Driver Interface Specification(NDIS2). This document shows you how
  to setup the driver and how to use the enhanced functions by setting the
  custom keywords in configuration file.


Contents of the Subdirectory:
=============================

    PCIND.DOS           The NDIS2 driver for Lan Requester DOS workstations.
    OEMSETUP.INF        The installation information file.
    LSDOS.TXT           This file.


Installation:
=============

  Before starting with the installation process, make sure that the adapter
  is properly installed and configured. You can use the diagnostic program
  (A:\SETUP.EXE) to make sure your connection with the network is correct.

  Installing driver procedure on DOS LAN Requester :
  -------------------------------------------------
      1) Install DOS Lan Requester to HardDisk with "NO Network Adapter
         Selected" option.

      2) Copy PCIND.DOS from your Driver diskette to DOS LAN Services
         subdirectory, like C:\NET .

      3) Under DOS LAN Requester subdirectory C:\NET, run INSTALL

      4) Move highlight to "The listed options are correct" item ,
         then press ENTER.

      5) Move highlight to "Network Card", then press ENTER.

      6) Select "Change driver for network card." item, then press ENTER.

      7) Select "Network card not shown in list below..", then press ENTER.

      8) Insert the PCI Ethernet driver diskette in floppy A,and specify
         the pathname A:\LANSVR40.DOS,then press ENTER.

      9) PCI Ethernet NDIS2 driver is now installed on your computer, reboot
         your computer.


  NOTE:
  -----
    Multiple Lan Adapters in a system:
      If you want to install mutiple Lan adapter in your system, you have to use
      the keyword, PCIID, in PROTOCOL.INI file to let driver locate the right
      adapter. And you must set DriverName to be PCIND$ and PCIND2$ for two
      different adapters.
      You can run A:\SETUP.EXE under DOS prompt to show all the
      Ethernet addresses of your adapters.


Configuration Files:
====================

    Sample of configuration file:
    -----------------------------
    (Suppose the Lan Requester package is installed at C:\NET directory)

    File Name:          C:\CONFIG.SYS
    ----------
        DEVICE=C:\NET\PROTMAN.DOS /I:C:\NET
        DEVICE=C:\NET\DLSHELP.SYS
        DEVICE=C:\NET\PCIND.DOS

    File Name:          C:\AUTOEXEC.BAT
    ----------
        SHARE
        C:\NET\NET START
        C:\NET\NET START PEER
        C:\NET\NET SHARE ZZZ=C:\

    File Name:          C:\NET\PROTOCOL.INI
    ----------
        ...
        # The followings are Custom Keywords. Put the keywords to enable the
        # special functions.
        [MS$PCIND]
        DriverName=PCIND$
        IOBASE=0x300
        INTERRUPT=5
        EARLYRECEIVE=0
        EARLYTRANSMIT=0
        FULLDUPLEX=0

        [MS$PCIND]
        DriverName=PCIND2$
        IOBASE=0x320
        INTERRUPT=9
        EARLYRECEIVE=0
        EARLYTRANSMIT=0
        FULLDUPLEX=0

        [IBM$NETBEUI]
        DriverName=netbeui$
        SESSIONS=20
        NCBS=20
        BINDINGS=MS$PCIND
        LANABASE=0
        ...


    Custom Keywords:
    ----------------
        PCIID="hhhhhhhhhhhh"            This keyword is the Ethernet Address of
                                        the adapter you want to drive. If there
                                        are more than one ethernet adapters in
                                        your system, you have to use this
                                        keyword to let driver locate the right
                                        adapter. However, you don't have to use
                                        this property or let the value to be
                                        zero (i.e. PCIID=0) if there is only
                                        one adapter in your system.

                                        Note: Please remember to enter the
                                              double quotes.

        EARLYTRANSMIT                   This keyword is used to enable turbo
                                        transmission mode for accelerating data
                                        transmission.

        EARLYRECEIVE                    This keyword is used to enable turbo
                                        transmission mode for accelerating data
                                        receiption.

        FULLDUPLEX                      This keyword is used to enable full
                                        duplex mode.

        Note: For PCI mode adapter, the IOBASE and INTERRUPT keywords values
              are ignored in your PROTOCOL.INI file.


