*****************************************************************************
*                                                                           *
*                         PCI Ethernet Adapter                              *
*                                                                           *
*                     NDIS3 Driver for Windows NT v3.5                      *
*                                                                           *
*                         V. 2.8,   May. 1996                               *
*                                                                           *
*****************************************************************************

Introduction:
=============

  This document shows you how to setup the driver and how to use the enhanced
  functions by setting the custom keywords.


Contents of the Subdirectory:
=============================

    PCIWNT.SYS          The NDIS3 driver for Windows NT.
    PCIWNT.HLP          The help file.
    OEMSETUP.INF        The setup information file.
    WINNT35.TXT         This file.


Installation:
=============

  Before starting with the installation process, make sure that the adapter
  is properly installed and configured.

    1. Open "Control Panel" -> "Networks", and choose the "Add Adapter" button.
       The Add Noetwork Adapter dialog box appears.  Select "<other> Requires
       disk from manufacturer" in the list of Network Adapters, and then press
       <Enter>.

    2. Insert the driver diskette into your floppy drive, and specify the
       path of the driver in the diskette(i.e. A:\WINNT35) if necessary.

    4. Select "PCI Ethernet Adapter", and start to copy the driver
       files to your system.

    5. After all the driver files have been copied to your system, a property
       dialog box appears in the screen. You can enable the special properties
       if you want to. Please refer to the next section to setup the properties.

    5. When the driver installation is completed, restart your PC.


Configuration Parameters:
=========================
    Configuration:
    --------------
      1) Open "Control Panel" -> "Networks", Press "Configure.." in the Netork
         Settings dialog box, and a property dialog box appear in the screen.

      2) You will see the following properties:
         EarlyReceive, EarlyTransmit, FullDuplex, and PCIID. Turn the properties
         on if you want to enable the functions.

    Custom Properties:
    ------------------
        EARLYTRANSMIT                   This property is used to enable turbo
                                        transmission mode for accelerating data
                                        transmission.

        EARLYRECEIVE                    This property is used to enable turbo
                                        receiption mode for accelerating data
                                        receiption.

        FULLDUPLEX                      This property is used to enable full
                                        duplex mode.

        PCIID = hhhhhhhhhhhh            This property is the Ethernet Address of
                                        the adapter you want to drive. If there
                                        are more than one ethernet adapters in
                                        your system, you have to use this
                                        property to let driver locate the right
                                        adapter. However, you don't have to use
                                        this property or let the value to be
                                        zero (i.e. PCIID = 0) if there is only
                                        one adapter in your system.


