************************************************************
** ENU *****************************************************
************************************************************
*                                                           
*  Intel(R) INF Installation Utility
*  Installation Readme
*                                                           
*  NOTE:  This document refers to systems containing the 
*         following Intel chipsets: 
*              Intel(R) 810  Chipset 
*              Intel(R) 810E Chipset 
*              Intel(R) 820  Chipset 
*              Intel(R) 840  Chipset 
*
*              Intel(R) 430TX PCIset 
*              Intel(R) 440BX AGPset 
*              Intel(R) 440DX AGPset 
*              Intel(R) 440EX AGPset 
*              Intel(R) 440GX AGPset 
*              Intel(R) 440LX AGPset 
*              Intel(R) 440MX Chipset 
*              Intel(R) 440ZX AGPset 
*
*
************************************************************
************************************************************


************************************************************
*  CONTENTS OF THIS DOCUMENT
************************************************************
This document contains the following sections:

1.  Overview
2.  Contents of the Distribution Package
3.  System Requirements
4.  Installing the Software
    4A. Installing the Software in Interactive Mode
    4B. Installing the Software in Silent Mode
5.  Verifying Installation of the Software
6.  Identifying the Software Version Number
7.  Troubleshooting


************************************************************
* 1.  OVERVIEW
************************************************************
The Intel(R) INF Installation Utility installs to 
the target system the Windows* INF files that outline to 
the operating system how the chipset components shall be 
configured.  This is needed for the proper functioning of
the following features:

   - Core PCI and ISAPNP Services
   - AGP Support
   - IDE/ATA33/ATA66 Storage Support
   - USB Support
   - Identification of Intel Chipset Components in 
     Device Manager


************************************************************
* 2.  CONTENTS OF THE DISTRIBUTION PACKAGE
************************************************************
The Intel(R) INF Installation Utility package contains the 
following items:

File(s)       
-------
INFINST_ENU.ZIP
README.TXT
RELNOTES.TXT

The version of the software included in the distribution
package is specified in the file RELNOTES.TXT.

RELNOTES.TXT is available in English only.

After installation on a Windows* 95 or Windows 98 system, 
one or more of the following INF files are copied 
to the <Windows>\INF directory:

File(s)
-------
440MXCOR.INF
440MXIDE.INF
440MXUSB.INF
810.INF
810B.INF
820.INF
820B.INF
840.INF
ICHx.INF
ICHxIDE.INF
ICHxSMB.INF
ICHxUSB.INF
IFWH.INF
IHOST.INF
P64H.INF
P64HRES.INF
PIIXXIDE.INF
PIIXXUSB.INF
PIIX4.INF


   *** NOTE:  Only the files that reference the currently 
              detected devices are copied to the system.

One or more of the following digital signature files are 
installed to the <Windows>\CATROOT directory on a 
Windows 98 system ONLY:

File(s)
-------
440MXCOR.CAT
440MXIDE.CAT
440MXUSB.CAT
810.CAT
820.CAT
820B.CAT
840.CAT
ICHx.CAT
ICHxIDE.CAT
ICHxSMB.CAT
ICHxUSB.CAT
IFWH.CAT
P64H.CAT
P64HRES.CAT


   *** NOTE:  Only the files that reference the currently 
              detected devices are copied to the system.


************************************************************
* 3.  SYSTEM REQUIREMENTS 
************************************************************
1.  The software included with this distribution package is 
    designed to operate with the following chipset 
    configurations:

          Intel(R) 810  Chipset
          Intel(R) 810E Chipset 
          Intel(R) 820  Chipset
          Intel(R) 840  Chipset

          Intel(R) 430TX PCIset 
          Intel(R) 440BX AGPset 
          Intel(R) 440DX AGPset 
          Intel(R) 440EX AGPset 
          Intel(R) 440GX AGPset 
          Intel(R) 440LX AGPset 
          Intel(R) 440MX Chipset 
          Intel(R) 440ZX AGPset 
      
2.  One of the following operating systems must be 
    installed on the system:
    Windows 95      4.00.950   (Original Release)
    Windows 95      4.00.950a  (OSR1)
    Windows 95      4.00.950b  (OSR2 without USB 
                                Supplement)
    Windows 95      4.00.950b  (OSR2.1 with USB 
                                Supplement)
    Windows 95      4.00.950c  (OSR2.5 with or 
                                without USB Supplement)
    Windows 98      4.10.1998  (Original Release)
    Windows 98 Second Edition
                    4.10.2222  (Original Release)
    Windows Millennium
                    4.90.2380  (Beta 1)
                              
3.  It is recommended that the software be installed on 
    systems with at least 32MB of system memory.

4.  It is recommended that there is sufficient hard disk 
    space in the <TEMP> directory (typically C:\WINDOWS\TEMP)
    on the system on which this software is installed.


Please check with your system provider to determine which 
operating system and Intel chipset are used in your system.  


************************************************************
* 4.  INSTALLING THE SOFTWARE 
************************************************************
This software can be installed in two modes: Interactive or 
Silent.  The Interactive Mode requires user input during
installation; the Silent Mode requires NO user input.


************************************************************
* 4A.  INSTALLING THE SOFTWARE IN INTERACTIVE MODE
************************************************************
1.  Check the System Requirements.  The operating system 
    must be fully installed and running on the system before
    running this software.

2.  Close any running applications. Otherwise, you may
    experience difficulties.

3.  Unzip the InstallShield* installation program files 
    into a temporary directory.

4.  Run the InstallShield installation program, SETUP.EXE.

5.  You will be prompted to agree to the license agreement.  
    If you do not agree, the Installer will exit before 
    extracting any files.
    
6.  Follow the on-screen instructions and use the default
    settings to complete the setup, once the operating
    system has rebooted.

7.  This completes the installation of the Intel(R) INF 
    Installation Utility.  


************************************************************
* 4B.  INSTALLING THE SOFTWARE IN SILENT MODE
************************************************************
1.  Check the System Requirements.  The operating system 
    must be fully installed and running on the system before 
    running this software.

2.  Close any running applications.  Otherwise, you may 
    experience some difficulties.

3.  Unzip the InstallShield* installation program files 
    into a temporary directory.

4.  Run the InstallShield installation program:
        SETUP.EXE -b -s  (for silent install with auto-reboot)
           - OR -
        SETUP.EXE -s     (for silent install without auto-reboot)

5.  The utility will perform the necessary updates and record
    the installation status in the following system registry 
    key:
        HKEY_LOCAL_MACHINE\Software\Intel\INFInst

6.  If the utility was invoked with the "SETUP -b -s" mode,
    the system will automatically reboot if the update was
    successful.

    NOTE:  The system MUST be rebooted for all device updates
           to take effect.

7.  To determine whether the install was successful, verify 
    the 'install' value in the registry key specified in Step 5.

    The following table describes the various parameter values:

    Value      Type      Data            Description
    ------     ----      ----            -----------
    install    String    "success"       The installation was successful.
                         "fail"          The installation was not successful.
                                         No INF files were copied to the 
                                         system.                

    reboot     String    "Yes"           A reboot is required to complete 
                                         the installation.
                         "No"            No reboot is required to complete 
                                         the installation.
                                
    version    String    <varies>        The current version number of the 
                                         Intel(R) INF Installation Utility


************************************************************
* 5.  VERIFYING INSTALLATION OF THE SOFTWARE
************************************************************
NOTE:  This procedure is common to Windows 98, Windows 98
Second Edition and Windows 95 systems.

Run Device Manager to verify the correct installation and
usage of the INF files.

1.  Click on Start
2.  Select Settings
3.  Select Control Panel
4.  Double-click on System icon
5.  Click on Device Manager tab
6.  Click on View devices by Connection button
7.  Click on Plug and Play BIOS, or 
    Advanced Configuration and Power Interface (ACPI) BIOS
8.  Click on PCI bus
9.  Check the descriptions for the following entries:

    *** NOTE:  If you see PCI standard ISA bridge you will need 
               restart your system and re-run the software.

    *** NOTE:  Device Manager will only display the names for devices         
               currently detected in the system.


    Intel(R) 82801AA I/O Controller Hub:
        Intel(r) 82801AA LPC Interface Controller 
        Intel(r) 82801AA Ultra ATA Controller 
        Intel(r) 82801AA USB Universal Host Controller 
        Intel(r) 82801AA SMBus Controller 
        Intel(r) 82801AA PCI Bridge 
        *** NOTE:  Depending on the system type, the 'AA' in the 
                   above five lines may be replaced by 'AB'


    Intel(R) 810 Chipset:
        Intel(r) 82810 System and Graphics Controller 
        -or-
        Intel(r) 82810 DC-100 System and Graphics Controller


    Intel(R) 810E Chipset:
        Intel(r) 82810e DC-133 System and Graphics Controller 


    Intel(R) 820 Chipset:
        Intel(r) 82820 Processor to I/O Controller
        Intel(r) 82820 Processor to AGP Controller


    Intel(R) 840 Chipset:
        Intel(r) 82840 Processor to I/O Controller 
        Intel(r) 82840 Processor to AGP Controller 
        Intel(r) 82840 PCI Bridge


    Intel(R) 82806AA PCI 64-bit Hub:
        Intel(r) 82806AA Advanced Programmable Interrupt Controller
        Intel(r) 82806AA PCI Bridge
        Intel(r) 82806AA Controller (reserved)

    
    Intel(R) 440MX Chipset:
        Intel(r) 82440MX Processor to I/O Controller
        Intel(r) 82440MX PCI to ISA Bridge
        Intel(r) 82440MX Power Management Controller
        Intel(r) 82440MX Bus Master IDE Controller
        Intel(r) 82440MX USB Universal Host Controller


    Intel(R) 82371AB Controller:
        Intel(r) 82371AB PCI to ISA bridge (EIO mode)
        Intel(r) 82371AB PCI to ISA bridge (ISA mode)
        Intel(r) 82371AB Power Management Controller
        Intel(r) 82371AB/EB/MB PCI Bus Master IDE Controller
        Intel(r) 82371AB/EB/MB PCI to USB Universal Host Controller
   

    Intel(R) 82371EB, 82371MB Controllers:
        Intel(r) 82371EB/MB PCI to ISA bridge (EIO mode)
        Intel(r) 82371EB/MB PCI to ISA bridge (ISA mode)
        Intel(r) 82371EB/MB Power Management Controller
        Intel(r) 82371AB/EB/MB PCI Bus Master IDE Controller
        Intel(r) 82371AB/EB/MB PCI to USB Universal Host Controller


    Intel(R) 82371SB Controllers:
        Intel(r) 82371SB PCI to ISA bridge
        Intel(r) 82371SB PCI Bus Master IDE Controller
        Intel(r) 82371SB PCI to USB Universal Host Controller


    Intel(R) 430TX PCIset:
        Intel(r) 82443TX Processor to PCI bridge


    Intel(R) 440BX AGPset, Intel(R) 440DX AGPset, Intel(R) 440ZX AGPset:
        Intel(r) 82443BX/ZX/DX Processor to PCI bridge
        Intel(r) 82443BX/ZX/DX Processor to AGP controller


    Intel(R) 440GX AGPset:
        Intel(r) 82443GX Processor to PCI bridge
        Intel(r) 82443GX Processor to AGP controller


    Intel(R) 440LX AGPset:
        Intel(r) 82443LX Processor to PCI bridge
        Intel(r) 82443LX Processor to AGP controller


10. On certain systems, the following device may also be
    updated:

    Intel(R) 810, Intel(R) 810E, Intel(R) 820, and Intel(R) 840 Chipset:

     a. Click on View devices by Connection button
     b. Click on Plug & Play BIOS, or
        Advanced Configuration and Power Interface (ACPI) BIOS     
     c. Verify that the following entry is present:
        Intel(r) 82802 Firmware Hub Device -OR-
        Intel(r) Security Driver

 
************************************************************
* 6.  IDENTIFYING THE SOFTWARE VERSION NUMBER
************************************************************
The version of the software included in the distribution
package is specified in the file RELNOTES.TXT.

RELNOTES.TXT is available in English only.


************************************************************
* 7.  TROUBLESHOOTING
************************************************************
It is assumed that the system requirements from Section 3
above have been satisfied.

Issue:      System locks up during Device Manager Remove or 
            during restart.

Solution:   System lockup can occur during Restart as a 
            result of several possible system issues.  In 
            the event of system lockup, restart the machine 
            and view Device Manager.  If devices are listed 
            properly and system experiences no further 
            problems, then .INF file restore process was 
            successful.  If devices are not configured 
            correctly try re-running the procedures outlined 
            in Section 4.

            If this does not fix problems or further 
            problems are experienced, re-install the 
            operating system.


Issue:      After running the setup program and rebooting the
            machine, Windows reports that it cannot find one 
            of the following files:
                  ESDI_506.pdr

Solution:   Click Browse in the dialog box where this problem
            occurs, locate the
                  <Windows>\System\IOSubsys

            directory and click OK.  The system should
            be able to locate this file in this directory 
            and continue re-enumerating for the new devices.

Issue:      After running the setup program and rebooting the
            machine, Windows reports that it cannot find one 
            of the following files:
 
                  UHCD.SYS
                  USBD.SYS
                  USBHUB.SYS

Solution:   Click Browse in the dialog box where this problem
            occurs, locate the
                  <Windows>\System32\drivers (for Windows 98)
                   -or-
                  <Windows>\System           (for Windows 95)

            directory and click OK.  The system should
            be able to locate this file in this directory 
            and continue re-enumerating for the new devices.

Issue:	    During setup, installation stops and prompts for one
	    of the following files:

		  UHCD.SYS
		  USBD.SYS
		  USBHUB.SYS

Solution:   Ensure that the Windows 95 USB Supplement has been 
	    installed prior to running the INF Installation Utility
	    setup program.

Issue:      After running the setup program and rebooting the
            machine, Windows reports that it cannot find one 
            of the following files:
                  isapnp.vxd

Solution:   Click Browse in the dialog box where this problem
            occurs, locate the
                  <Windows>\System

            directory and click OK.  The system should
            be able to locate this file in this directory 
            and continue re-enumerating for the new devices.

Issue:      After performing the silent install, the 
            HKLM\Software\Intel\InfInst key was not created 
            or the data of the value "install" is not 
            "success".

Solution:   This is caused by one of the following scenarios:
               - the current system does not contain 
                 a supported operating system, or
               - the current system does not contain 
                 a supported chipset

            Verify the System Requirements in Section 3.


************************************************************
************************************************************
* DISCLAIMER
************************************************************
Intel is making no claims of usability, efficacy or 
warranty.  
The INTEL SOFTWARE LICENSE AGREEMENT
(OEM / ISV Distribution & Single User) 
completely defines the licensed use of this software.
************************************************************
Information in this document is provided in connection with 
Intel products.  No license, express or implied, by estoppel 
or otherwise, to any intellectual property rights is granted 
by this document.  Intel assumes no liability whatsoever, 
and Intel disclaims any express or implied warranty, 
relating to sale and/or use of Intel products including 
liability or warranties relating to fitness for a particular 
purpose, merchantability, or infringement of any patent, 
copyright or other intellectual property right.  Intel 
products are not intended for use in medical, life saving, 
or life sustaining applications.

************************************************************
Intel Corporation disclaims all warranties and liabilities 
for the use of this document and the information contained 
herein, and assumes no responsibility for any errors which 
may appear in this document, nor does Intel make a 
commitment to update the information contained herein. Intel 
reserves the right to make changes to this document at any 
time, without notice.
************************************************************
************************************************************

* Third-party brands and names are the property of their 
respective owners.

Copyright (c) Intel Corporation, 1997-1999

