This nForce WinXP/win2K driver package contains the below components:


Ethernet Driver (v65.65) WHQL
SMBus Driver (v4.60) WHQL
Installer (v5.48)
IDE SataRAID Driver (v10.1.0.12) WHQL
IDE SataIDE Driver (v10.1.0.12) WHQL
RAIDTOOL Application (v10.1.0.12)
Display Driver (v101.17) WHQL
SMU (v1.31) WHQL

Fixed Issue

- Problem :  F6 Install of WinXP 32/64 storage driver on MCP68 with AHCI mode results in a non-WHQL warning message dispalayed 
- Root cause :  There was a cat file mismatch between the txtsetup.oem and the inf file.


Known Issue

- (Storage)Systems Hangs during shutdown if boot array is in degraded state. The shutdown logo spins for a little while and then the system hangs at splash screen. 
There is no BSOD.  If you Re-init system it will come up normally without risk of data loss. Only shutdown is affected.
This problem has been root caused and will be corrected in the next release

- (Installer) On uninstalling the Network driver the N/W device disappears in the device manager.  The network device comes back normally 
  on reinstallation of the driver with the S/W package.