MOTOROLA

Driver Installation:

On starting Windows for the first time after installing the SM56 AC-L modem, 
the Plug and Play (PnP) sub-system detects the new hardware and begins an install 
wizard for the modem. The SM56 AC-L modem is detected as a new PCI Device. The wizard 
fist looks for the modem information (INF) file, which is included on Installation CD. 
This file contains information about the modem, including device type, device driver 
information, as well as the AT command/response sets that it supports.

Browse to the SM56 AC-L modem files on the Installation CD. Windows will find the 
information on the disk. On Windows 95 and older versions of Windows 98 you may get an 
error message Cannot Locate File...... If you do, simply repoint the install wizard to 
the Installation CD and it will find the file the second time around.

Windows copies the necessary modem files to the computer. After modem installation is 
complete, Windows reports the SM56 AC-L modem in the Control Panel and Device Manager.

For D/F/TAM and D/F/TAM/Speakerphone modems, Windows finds a second device after the modem 
has been installed. Windows notifies you that it has found a Serial Wave Device for the 
modem and prompts for a Wave Device driver. Re-point to the Installation CD and click 
OK. It finds the INF file and installs the appropriate drivers. 
