#
# format for txtsetup.oem.
#
# General format:
#
# [section]
# key = value1,value2,...
#
#
# The hash ('#') introduces a comment.
# Strings with embedded spaces, commas, or hashes should be double-quoted
#


# This section lists all disks in the disk set.
#
# <description> is a descriptive name for a disk, used when
#   prompting for the disk
# <tagfile> is a file whose presence allows setup to recognize
#   that the disk is inserted.
# <directory> is where the files are located on the disk.
#

[Disks]

d1 = "VIA RAID Combo Driver Diskette", \RAID\winxp\VIAMRAID.SYS, \RAID\winxp
d2 = "VIA RAID Combo Driver Diskette", \RAID\win2000\VIAMRAID.SYS, \RAID\win2000
d3 = "VIA RAID Combo Driver Diskette", \RAID\Winnt40\VIAMRAID.SYS, \RAID\Winnt40
d4 = "VIA RAID Combo Driver Diskette", \RAID\2003ia32\VIAMRAID.SYS, \RAID\2003ia32
#d9 = "VIA RAID Combo Driver Diskette", \RAID\x64\VIAMRAID.SYS, \RAID\x64

d5 = "VIA ATA/ATAPI Host Controller Driver", \PIDE\winxp\viapdsk.sys, \PIDE\winxp
d6 = "VIA ATA/ATAPI Host Controller Driver", \PIDE\win2000\viapdsk.sys, \PIDE\win2000
d7 = "VIA ATA/ATAPI Host Controller Driver", \PIDE\winnt40\viapdsk.sys, \PIDE\winnt40
d8 = "VIA ATA/ATAPI Host Controller Driver", \PIDE\2003ia32\viapdsk.sys, \PIDE\2003ia32

# This section lists the default selection for each 'required'
# hardware component.  If a line is not present for a component,
# the default defaults to the first item in the [<component_name>]
# section (see below).
#
# <component_name> is one of computer, display, keyboard, mouse, scsi
# <id> is a unique <within the component> string to be associated
#   with an option.

[Defaults]

scsi = VIARAID_MULTIPLE_XP


# This section lists the options available for a particular component.
#
# <id> is the unique string for the option
# <description> is a text string, presented to the user in a menu
# <key_name> gives the name of the key to be created for the component in
#   HKEY_LOCAL_MACHINE\ControlSet001\Services

[scsi]
VIARAID_MULTIPLE_2003IA32 = "VIA RAID Controller(Windows 2003 IA32)"
VIARAID_MULTIPLE_XP = "VIA RAID Controller(Windows XP)"
VIARAID_MULTIPLE_2K = "VIA RAID Controller(Windows 2000)"
VIARAID_MULTIPLE_NT = "VIA RAID Controller(Windows NT4)"
#VIARAID_MULTIPLE_2003K864 = "VIA RAID Controller(Windows 2003 AMDx86-64)"

VIAPDSK_VT4149_2003IA32 = "VIA ATA/ATAPI Host Controller(Windows 2003IA32)"
VIAPDSK_VT4149_XP = "VIA ATA/ATAPI Host Controller(Windows XP)"
VIAPDSK_VT4149_2K = "VIA ATA/ATAPI Host Controller(Windows 2000)"
VIAPDSK_VT4149_NT = "VIA ATA/ATAPI Host Controller(Windows NT4)"

# This section lists the files that should be copied if the user
# selects a particular component option.
#
# <file_type> is one of driver, port, class, dll, hal, inf, or detect.
#   See below.
# <source_disk> identifies where the file is to be copied from, and must
#   match en entry in the [Disks] section.
# <filename> is the name of the file. This will be appended to the
#   directory specified for the disk in the [Disks] section to form the
#   full path of the file on the disk.
#=======================================#

[Files.scsi.VIARAID_MULTIPLE_XP]
driver = d1, viamraid.sys, VIAMRAID_NT5
inf = d1, viamraid.inf
## Cat file directive. It should be marked with non-digital signed driver
catalog = d1, viamraid.cat

[Files.scsi.VIARAID_MULTIPLE_2K]
driver = d2, viamraid.sys, VIAMRAID_NT4
inf = d2, viamraid.inf
## Cat file directive. It should be marked with non-digital signed driver
catalog = d2, viamraid.cat

[Files.scsi.VIARAID_MULTIPLE_NT]
driver = d3,viamraid.sys,VIAMRAID_NT4
inf = d3,viamraid.inf

[Files.scsi.VIARAID_MULTIPLE_2003IA32]
driver = d4, viamraid.sys, VIAMRAID_NT5
inf = d4, viamraid.inf
## Cat file directive. It should be marked with non-digital signed driver
catalog = d4, viamraid.cat

#[Files.scsi.VIARAID_MULTIPLE_2003K864]
#driver = d9, viamraid.sys, VIAMRAID_NT5
#inf = d9, viamraid.inf

#[HardwareIds.scsi.VIARAID_MULTIPLE_2003K864]
#id = "PCI\VEN_1106&DEV_3249","viamraid"
#id = "PCI\VEN_1106&DEV_3149","viamraid"
#id = "PCI\VEN_1106&DEV_3164","viamraid"

[HardwareIds.scsi.VIARAID_MULTIPLE_2003IA32]
id = "PCI\VEN_1106&DEV_3249","viamraid"
id = "PCI\VEN_1106&DEV_3149","viamraid"
id = "PCI\VEN_1106&DEV_3164","viamraid"

[HardwareIds.scsi.VIARAID_MULTIPLE_XP]
id = "PCI\VEN_1106&DEV_3249","viamraid"
id = "PCI\VEN_1106&DEV_3149","viamraid"
id = "PCI\VEN_1106&DEV_3164","viamraid"

[HardwareIds.scsi.VIARAID_MULTIPLE_2K]
id = "PCI\VEN_1106&DEV_3249","viamraid"
id = "PCI\VEN_1106&DEV_3149","viamraid"
id = "PCI\VEN_1106&DEV_3164","viamraid"


# This section lists the files that should be copied if the user
# selects a particular component option.
#
# <file_type> is one of driver, port, class, dll, hal, inf, or detect.
#   See below.
# <source_disk> identifies where the file is to be copied from, and must
#   match en entry in the [Disks] section.
# <filename> is the name of the file. This will be appended to the
#   directory specified for the disk in the [Disks] section to form the
#   full path of the file on the disk.
#=======================================#

[Files.scsi.VIAPDSK_VT4149_XP]
driver = d5, viapdsk.sys, VIAMRAID_NT5
inf = d5, viapide.inf
## Cat file directive. It should be marked with non-digital signed driver
catalog = d5, viapdsk.cat

[Files.scsi.VIAPDSK_VT4149_2K]
driver = d6, viapdsk.sys, VIAMRAID_NT4
inf = d6, viapide.inf
## Cat file directive. It should be marked with non-digital signed driver
catalog = d6, viapdsk.cat

[Files.scsi.VIAPDSK_VT4149_NT]
driver = d7, viapdsk.sys, VIAMRAID_NT4
inf = d7, viapide.inf

[Files.scsi.VIAPDSK_VT4149_2003IA32]
driver = d8, viapdsk.sys, VIAMRAID_NT5
inf = d8, viapide.inf
## Cat file directive. It should be marked with non-digital signed driver
catalog = d8, viapdsk.cat

[HardwareIds.scsi.VIAPDSK_VT4149_2003IA32]
id = "PCI\VEN_1106&DEV_4149","viapdsk"

[HardwareIds.scsi.VIAPDSK_VT4149_XP]
id = "PCI\VEN_1106&DEV_4149","viapdsk"

[HardwareIds.scsi.VIAPDSK_VT4149_2K]
id = "PCI\VEN_1106&DEV_4149","viapdsk"

#===============================================================================
# This section specifies values to be set in the registry for
# particular component options.  Required values in the services\xxx
# key are created automatically -- use this section to specify additional
# keys to be created in services\xxx and values in services\xxx and
# services\xxx\yyy.
#
# <key_name> is relative to the services node for this device.
#   If it is empty, then it refers to the services node.
#   If specified, the key is created first.
# <value_name> specifies the value to be set within the key
# <value_type> is a string like REG_DWORD.  See below.
# <value> specifies the actual value; its format depends on <value_type>

[Config.VIAMRAID_NT5]
value = Parameters\PnpInterface, 5, REG_DWORD, 1

[Config.VIAMRAID_NT4]
value = "", Tag, REG_DWORD, 1

