Sil 3114 SATARaid 
RAID Controller Adapter
Silicon Image  
 
 
Tested and Approved with the following Novell products: 
NetWare 6 NetWare 6.5 

Product Description 
Sil 3114 SataLink/Raid HAM, 4 Channel, with built in Raid 0, 1 & 0+1.  

Primary Driver File(s) 
SI3114.HAM (103778 bytes 10-Mar-2004 08:03 am v2.01d)  

Driver Support File(s) 
SI3114.DDI (19548 bytes 08-Mar-2004 04:16 pm v2.14)  

Test Configuration 
Product Name Sil 3114 SATARaid  
CD-ROM Drive Intel® CDU5211; Firmware YYS7; ATAPI  
Hard Disk Drive Silicon Image RAID 0 Set; 163. GB; Firmware 2.10; Serial ATA 150 (SATA150)  
 Silicon Image RAID 1 Set; 81.9 GB; Firmware 2.10; Serial ATA 150 (SATA150)  
Host Bus Adapter Silicon Image Sil 3114; PCI; BIOS 2.01.04; Channels 4; Chipset 1095.3114; Firmware n/a; Serial ATA 150 (SATA150); PCI.1095.3114.1095.6114.02; Version n/a  
System Intel® Vero Beach; Xeon(TM) CPU 2.40GHz ; BIOS Phoenix 4.0 Release 6.0 08/15/03; PCI-ISA; Memory 512 MB  

Configuration Note(s) 
The IDE/ATA interface does not support fault tolerance.  
Vero Beach requires MPS14.PSM Ver 3.00 April 11, 2003.   

The term Tested and Approved applies only to the exact configuration documented in this bulletin. For more information regarding the specific test configuration, please contact:  

Silicon Image 
1060 E Arques Ave 
Sunnyvale, CA 94085 
