
                  MR8800-U Data+Fax Modem 
                  =======================

MR8800-U is a Modem Riser card.

Section 1: Important Information
Section 2: Installation under Win98
Section 3: Additional Information
Section 4: Uninstalling of Modem

--------------------------------------------------------------------------

Section 1:      Important Information
=====================================

System Requirements
-------------------
    .   Minimum system requires a Pentium Celeron CPU and 32MB of system RAM operating under
	Windows 95/98 environment with CD-ROM drive.

    .   WinNT4.0 and Windows 2000  drivers are still in development state and is not available
        at the time this product was release for evaluation.



Section 2:      Installation under Windows 98
=============================================

Plug & Play Driver Installation
-------------------------------

MR8800 is Windows PnP device.

    For Windows 98 (Version 4.10.1998) & Windows .
    ---------------------------------------------

    1.  OS will automatically detect "MR8800 Modem".  Click "Next" to continue.

    2.  Insert the Installation CD provided into the Cdrom Drive.

    3.	Select "Search for the best drivers for your device. (Recommended)"
        and click "Next" to continue.

    4.	Enable "CD-Rom drive" selection and click "Next" to continue.

    5.  Modem Driver will be found in the Installation CD.  Click "Next" to
        continue.

    6.  Click "Finish" to complete MR installation.

--------------------------------------------------------------------------

Section 3:      Additional Information
======================================


How to install Microsoft Fax in Windows 98?
-------------------------------------------

    If you are staying in US, go to directory  D:\Tools\oldwin95\message\us in 
    Windows 98 installation CD.  For other countries go to 
    D:\Tools\oldwin95\message\intl 

    1.	First run wms.exe under the directory to install Microsoft Messaging.

    2.	Next run awfax.exe under the same directory to install Microsoft Fax.

    For further information on Microsoft Messaging and Microsoft Fax, read
    wms-fax.txt under the same directory in Windows 98 CD.


--------------------------------------------------------------------------

Section 4:      Uninstalling of Modem
=====================================

HOW TO UNINSTALL MR8800?
------------------------

    To uninstall and remove modem completely from the system, proceed to 
    double click on the "Uninstall MR8800 Modem" under Control Panel | 
    Add/Remove Program icon.

    To complete the uninstallation, you need to run/remove both "Uninstall 
    MR8800 Modem" entries.


--------------------------------------------------------------------------

    If you encounter some resource conflicts after loading the modem device, 
    please refer to Trouble-shooting section in Windows 98 for further
    details.



	***********************************************************
	*   In case you encounter any problem with our products,  *
	*   please quote the following model(s) when calling our  *
	*   Technical Support :					  *
	*					MR8800 Modem	  *
	***********************************************************


 
			  -------  The End  ---------
