

    1. Make one temporary directory in your harddisk.
    2. Unzip the ZIP file into the temporary directory.
    3. Run FLASHCOM.EXE from Win 95/98 system.
    4. The utility will detect modem automatically.
    5. Highlights the COM port with "flash-loadable" message.
       Then, click "Load Now" start the download procedure.
    6. Wait about 1 or 2 minutes for the utility to complete the download
       procedure. Please don't turn off modem power during this period.
       Otherwise, the content of Flash EPROM will be destroy.

