
 REM PCMCIA LS-120 DRIVER
 REM MUST BE PRESENT AFTER CARD/SOCKET SERVICES
 REM INSTALLED BY COMMUTER UTILITY

DEVICEHIGH=C:\COMMUTER\PATAPISF.SYS
