*******************************************
DCB201 Windows 2000 Driver Release Notes
*******************************************


Files Included With This Distribution:
______________________________________

usbstor.sys
usbstor.inf
readme.txt



Installation Instructions:
______________________________________

1. Plug the DCB201 device into a free USB 1.1 or 2.0 port on the host.

2. Windows 2000 will automatically load it's own mass storage class driver. Once the device has been enumerated, you will only see 1 icon is Windows Explorer. This is because the Windows 2000 native mass storage class driver does not provide support for multiple LUN devices like the DCB201

3. Go to the Device Manager and expand the "Universal Serial Bus Controllers" branch by clicking the "+" sign to the left of it.

4. Look for an entry under Universal Serial Bus Controllers called "USB Mass Storage Device". Caution: If you have a USB hard drive, USB floppy drive or some other USB mass storage class device attached to your system, 
you will see more than one "USB Mass Storage Device" entry. If possible, 
you should unplug these devices to avoid any confusion.

5. Once you have identified the USB Mass Storage Device entry for the DCB201 device, double click it to bring up the "Driver Properties" dialog.

6. Click the "Driver" tab at the top, and then click the "Update Driver" button. This will start the "Upgrade Device Driver" wizard.

7. Follow the Update Device Driver wizard, and when asked for the location of the driver, select the "Specify Location" check box and click "Next".

8. Browse to the location of the DCB201 Windows 2000 installation files, select "OK" and then keep clicking the "Next" button until you get to the "Finish" dialog. Press "Finish" to complete the installation.

9. You can now go to Windows Explorer, and you should see one drive icon for each supported flash media type.




Architecture and Capabilities:
______________________________________

1. WDM based architecture
2. Supports up to 16 LUNs
3. Supports only BULK-ONLY Protocol devices




