
*******************************************
DCB201 Windows 98 Driver Release Notes
*******************************************


Files Included With This Distribution:
______________________________________

usbatap1.inf
usbatap2.inf
umsspdr.pdr (Port Driver)
masswdm.sys (WDM Driver)



Installation Instructions:
______________________________

1. Plug the DCB201 device into a free USB 1.1 or 2.0 port on the host.

2. The "Found New Hardware" wizard will appear. Follow the instructions, and when prompted for the location of the driver, select "Specify Location".

3. Browse to the location of the DCB201 Windows 98 Driver installation files(this directory) and press "OK".

4. Once you complete the Found New Hardware wizard, and the driver has loaded, you can open Windows Explorer and you should see 1 drive icon for each supported flash media type.




Architecture and Capabilities:
______________________________________

1. WDM based architecture
2. Supports only BULK-ONLY Protocol devices




