[Version]
Signature="$CHICAGO$"
Class=USB
;//---0509 2003
ClassGUID=%VERSIONPAGE%
;//---0509 2003
provider=%GENERIC%
LayoutFile=LAYOUT.INF
DriverVer=12/15/2000,5.00.2195.1

[ControlFlags]
ExcludeFromSelect = *

[Manufacturer]
%MfgName%=GENERICDevs

[GENERICDevs]
%USB\VID_0DDA&PID_0001.DeviceDesc%=USBARW,USB\VID_0DDA&PID_0001
%USB\VID_0DDA&PID_0002.DeviceDesc%=USBARW,USB\VID_0DDA&PID_0002
%USB\VID_0DDA&PID_0005.DeviceDesc%=USBARW,USB\VID_0DDA&PID_0005
%USB\VID_0DDA&PID_000A.DeviceDesc%=USBARW,USB\VID_0DDA&PID_000A
%USB\VID_0DDA&PID_0101.DeviceDesc%=USBARW,USB\VID_0DDA&PID_0101
%USB\VID_0DDA&PID_0102.DeviceDesc%=USBARW,USB\VID_0DDA&PID_0102
%USB\VID_0DDA&PID_0302.DeviceDesc%=USBARW,USB\VID_0DDA&PID_0302
%USB\VID_0DDA&PID_2001.DeviceDesc%=USBARW,USB\VID_0DDA&PID_2001
%USB\VID_0DDA&PID_2003.DeviceDesc%=USBARW,USB\VID_0DDA&PID_2003
%USB\VID_0DDA&PID_2005.DeviceDesc%=USBARW,USB\VID_0DDA&PID_2005
%USB\VID_0DDA&PID_2006.DeviceDesc%=USBARW,USB\VID_0DDA&PID_2006
%USB\VID_0DDA&PID_2007.DeviceDesc%=USBARW,USB\VID_0DDA&PID_2007
%USB\VID_0DDA&PID_2008.DeviceDesc%=USBARW,USB\VID_0DDA&PID_2008
%USB\VID_0DDA&PID_2013.DeviceDesc%=USBARW,USB\VID_0DDA&PID_2013
%USB\VID_0DDA&PID_2014.DeviceDesc%=USBARW,USB\VID_0DDA&PID_2014
%USB\VID_0DDA&PID_2026.DeviceDesc%=USBARW,USB\VID_0DDA&PID_2026
%USB\VID_0DDA&PID_2027.DeviceDesc%=USBARW,USB\VID_0DDA&PID_2027

[PreCopySection]
HKR,,NoSetupUI,,1

[DestinationDirs]
USBARW.CopyList = 10, system32\drivers

[USBARW.NT]
CopyFiles=USBARW.CopyList

[USBARW.HW]
AddReg=USBARW.HW.AddReg

[USBARW.HW.AddReg]
HKR,,upperfilters,0,"NTMAP.SYS"

[USBARW.NT.Services]
Addservice = USBARW, 0x00000002, USBARW.AddService

;//---0509 2003
[USBARW.AddReg]
HKLM,"SYSTEM\CurrentControlSet\Control\Class\{36FC9E60-C465-11CF-8056-444553540000}","EnumPropPages32",0x00000,storpg2k.dll

[USBARW.NT.HW]
AddReg=DriverHwAddReg

[DriverHwAddReg]
HKR,,DriverVersion,,"V1.0"
HKR,,FirmwareBCD,,"V1.0"

;HKEY_LOCAL_MACHINE\SYSTEM\ControlSet001\Services\USBARW
;HKEY_LOCAL_MACHINE\SYSTEM\ControlSet001\Enum\USB\Vid_0dda&Pid_0001\2001-77\Device Parameters
;//---0509 2003

[USBARW.AddService]
DisplayName    = %USBARW.SvcDesc%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\USBARW.SYS

AddReg=USBARW.AddReg

[USBARW.CopyList]
;USBARW.SYS

[Strings]
GENERICName="GENERIC"
MfgName="GENERIC"

USB\VID_0DDA&PID_0001.DeviceDesc="Multi-Card Reader 6in1"
USB\VID_0DDA&PID_0002.DeviceDesc="Multi-Card Reader 7in1"
USB\VID_0DDA&PID_0005.DeviceDesc="Internal Multi-Card Reader 6in1"
USB\VID_0DDA&PID_000A.DeviceDesc="MS+SD Dual Card Reader"
USB\VID_0DDA&PID_0101.DeviceDesc="All-In-One Card Reader"
USB\VID_0DDA&PID_0102.DeviceDesc="All-In-One Card Reader"
USB\VID_0DDA&PID_0302.DeviceDesc="Multi-Card MP3 Player"
USB\VID_0DDA&PID_2001.DeviceDesc="Multi-Card Reader"
USB\VID_0DDA&PID_2003.DeviceDesc="Multi-Card Reader"
USB\VID_0DDA&PID_2005.DeviceDesc="Multi-Card Reader"
USB\VID_0DDA&PID_2006.DeviceDesc="All-In-One Card Reader"
USB\VID_0DDA&PID_2007.DeviceDesc="USB 2.0 to ATAPI bridge"
USB\VID_0DDA&PID_2008.DeviceDesc="All-In-One Card Reader"
USB\VID_0DDA&PID_2013.DeviceDesc="USB 2.0 SD/MS Combo Card Reader"
USB\VID_0DDA&PID_2014.DeviceDesc="USB 2.0 SD/MS Single Card Reader"
USB\VID_0DDA&PID_2026.DeviceDesc="USB 2.0 card reader DEMO board with ICSI brand name (MaskROM version)"
USB\VID_0DDA&PID_2027.DeviceDesc="USB 2.0 card reader DEMO board with Generic brand name (MaskROM version)"
USBARW.SvcDesc = "=USB Mass Storage Disk Driver="

;//---0509 2003
VERSIONPAGE	="{36FC9E60-C465-11CF-8056-444553540000}"
;//---0509 2003
