Feature :
=========

  - Can be used for 6in1, 7in1, Flash Disk, Multi-Falsh Disk


Update Issue :
==============

  V2.01.0119
  --------------
  - For supporting SM/xD combined icon, change icon SM, xD to SM/xD combo icon. change dit.dll group 17,27 icon to XD/SM.
  - Bug fix of dix.exe
  - Change description of PID 2026, 2027 to as following.
  - Icon works after installation program.

 
  V2.00.1215
  --------------
  - Win98 Driver V2.09, Win2K Driver V3.05
  - Keep Icon Infomation during LogOut and LogIn.
  - Support COMBO CardReader ("B1" and "B2").
  - Add some VID&PID below:

        VID:0DDA
        ========
        PID     Name                       Use native driver in Win2000
        ===============================================================
	2013	USB 2.0 SD/MS Combo Card Reader	   	   N
	2014	USB 2.0 SD/MS Single Card Reader	   N
	2026	USB 2.0 card reader DEMO board with ICSI brand name (MaskROM version)  N
	2027	USB 2.0 card reader DEMO board with Generic brand name (MaskROM version)   N

  V2.00.1205
  --------------
  - Win98 Driver V2.09, Win2K Driver V3.05
  - No authorization problem for Customized Icon in WinXP.
  - Customized Icon don't remain after boot.
  - Customized Icon refresh properly after boot, S3 and S4.

  V2.00.1114
  --------------
  - Win98 Driver V2.09, Win2K Driver V3.05
  - Improve Customized Icon in WinXP

  V2.00.0829
  --------------
  - Win98 Driver V2.09, Win2K Driver V3.05
  - for USBISP2.0

  V2.00.0716
  --------------
  - Win98 Driver V2.08, Win2K Driver V3.04
  - Fix : LED twinkles in Win2K.
  - Fix : Icon disappear after suspend in Win98
  - Add 32x32 and 16x16 True-Color Icon
  - More stable icon in WinXP.
  - Fix : GRAYIFNOCARD no effect.
  - Fix : Customized Icon Conflict with ONs.
  - Fix : Icon not appear if card write-protected.
  - Fix : Unstable for I-Code FlashDisk


  V1.99.0609
  --------------
  - Win98 Driver V2.08, Win2K Driver V3.03
  - Modify Readme.txt, add files list:

    Package Files:
	win2k:
	  - USBARW.SYS   		V3.03		
	  - ICSI2K.INF
	  - storpg2k.dll				for property page to display driver and firmware (bcd) version

	win98:
	  - USBSYS9X.SYS		V2.08 		 
	  - USBDSK9X.PDR
	  - ICSI98.INF   		 		 
 	  - icsi98pr.inf
	  - storpg98.dll		 		for property page to display driver and firmware (bcd) version

    This version extends the existing one by:
      In win2k:
	1) Support property page to display driver and firmware (bcd) version.

	   Update parts:
	   a.copy the storpg2k.dll to windows\system32
	   b.update icsi2k.inf
	   c.update usbarw.sys
		
	   ,ie,	USBARW.SYS => <WINDIR>\System32\Drivers
		ICSI2K.INF => <WinDIR>\Inf
		storpg2k.dll => <WINDIR>\System32
      In win98:	
 	1) Support property page to display driver and firmware (bcd) version.
	2) Divide the original icsi98.inf to two files, icsi98.inf and icsi98pr.inf.
	2) Fix: After rejecting disk, disk could not be accessed until repluging in the disk 
	   	after the second times. (for removeable disk)
	   	PS.This driver is also compatible with Msys dirver.(98 v2.07)  

    	   Update parts:
 	   a.copy the storpg98.dll to windows directory
 	   b.update icsi98.inf (windows\inf)
 	   c.update icsi98pr.inf (windows\inf)
 	   d.update usbsys9x.sys
 	   e. the usbdsk9x.pdr is same with preview version.

	   ie,  USBSYS9X.SYS => <WinDIR>\System32\Drivers
		USBDSK9X.PDR => <WinDIR>\System\IOSubSys
		ICSI98.INF => <WinDIR>\Inf
		icsi98pr.inf  => <WinDIR>\Inf
		storpg98.dll => <WinDIR>


  V1.99.0603
  --------------
  - Win98 Driver V2.08, Win2K Driver V3.03
  - Support property page to display driver and firmware (bcd) version.
  - Divide the original icsi98.inf to two files, icsi98.inf and icsi98pr.inf.
  - Fix: After rejecting disk, disk could not be accessed until repluging in the disk 
    after the second times. (for removeable disk)
    PS.This driver is also compatible with Msys dirver.(98 v2.07)  


  V1.99.0522
  --------------
  - Win98 Driver V2.06, Win2K Driver V3.02
  - Add some VID&PID below:

        VID:0DDA
        ========
        PID     Name                       Use native driver in Win2000
        ===============================================================
        0101    All-in-one card reader     N
	0102	All-in-one card reader	   N
	2008	All-in-one card reader	   N
	2006	All-in-one card reader	   N
	2007	USB 2.0 to ATAPI bridge	   N


  V1.99.0519
  --------------
  - Win98 Driver V2.06, Win2K Driver V3.02
  - Fix the bug of being not able to access disk again after rejecting disk for Win98.
  - Show Color Icon always for USB1.1 Device.


  V1.99.0515
  --------------
  - Win98 Driver V2.05, Win2K Driver V3.02
  - Add PIDs below : 2001,2003,2005,2006,2007


  V1.99.0506
  --------------
  - Win98 Driver V2.05, Win2K Driver V3.01
  - USB1.1/2.0 CardReader/FlashDisk Driver!
  - Driver can be installed repeatedly by adding new VID/PID into INF files
  - Show "Welcome" instead of "Maintain" if install ths driver AGAIN
  - Support gray-level icon if no card inserted.
  - Support icon changed when card insert/remove


  V1.20.0219
  --------------
  - Fix some issue for customized icon


  V1.20.0116
  --------------
  - Support SCSI pass through in 98 and 2K Driver
  - Fix some issue for 98 and 2K Driver
  - Add xD customer icon support
  - Add internal 6-in-1 card reader PID(0005) support


  V1.12.1209
  --------------
  - Fix some issue in USBARW.SYS
  - Support 48*48 Driver Icon in WinXP SP1


  V1.11.1127
  --------------
  - Win2000 driver update : SimboleLink Name Multi-Plug-in-out.
  - Win2000 driver update : "Combo disk" name to Inquiry data.
  - Show more correct driver Icon in Win98 
  - Add uninstall shortcut in program files


  V1.10.1008
  --------------
  - Add some VID&PID below:

        VID:0DDA
        ========
        PID     Name                       Use native driver in Win2000
        ===============================================================
        0001    Multi-Card Reader 6in1     N
        0002    Multi-Card Reader 7in1     N
        0003    Flash Disk                 Y
        0008    SD Single Card Reader      Y
        0009    MS Single Card Reader      Y
        000A    MS+SD Dual Card Reader     N
        000B    SM single Card Reader      Y
        0301    MP3 Player                 Y
        0302    MultiCard MP3 Player       N
        1001    Multi-Flash Disk           Y


  V1.10.0905
  --------------
  - Color Drive Icon
  - Show correct Drive Icon in some critical state
  - Use native driver for Win2000/SP3 or later.


  V1.10.0801
  ----------
  - For WinXP : The autorun.inf and icon file will NOT be copied into cards
  - For WinXP : Icons appear only for Service Pack 1 of WinXP


  V1.10.0712
  ----------
  - For WinXP : No Error Message for Write-Protect card
  - For WinXP : Hidden attribute for autorun.inf and icon file
  - For WinXP : Icon appears after formatting card


  V1.10.0702
  ----------
  - Bug Fix : Error Msg of "Program can not be initial" when rebooting
  - Bug Fix : No Customized Icon after mouse-right-button of "Eject card"
  - VID_0DDA&PID_0003 doesn't include in ICSI2K.INF


  V1.10.0625
  ----------
  - Win98 and Win2K Driver Update
    = Fixed the USB-ISP high failure rate
    = Fixed the suspend issue when copying file in Win2K
  - Icon on XP (Only on Flash and the drivers that cards plug-in)
  - Bug fix : Icon can not work after reboot with plug-in card reader.
  - Customized INF Filename
  - Customized UI String
  - Customized IconDLL File without CRC error
  - Bug fix : GPF on Shell32.dll during installation