
1.0 Install the Windows 95 with WinFast 3D L2300 board in the PC

    Install Windows 95 in the usual way. When installation has
    completed, Windows 95 should be booted on the VGA. Follow the
    section 1.1 "Fitting WinFast 3D L2300 board with Windows 95
    already installed" to install the drivers of WinFast 3D L2300.

1.1 Fitting WinFast 3D L2300 board with Windows 95 already installed

    During the booting of Windows 95, a message "New hardware Found
    PCI XGA Compatible Adapter" of "New hardware Found PCI VGA Compatible
    Adapter" must be shown on the screen. This represents Windows 95 can not
    locate the device driver(s) of WinFast 3D L2300.
    Follow the procedure below:

    Step 1   Insert the "Windows 95 Display Driver Disk 1" diskette into
             floppy drive A.
    Step 2   Select the "Driver from Disk Provided by Hardware Manufacturer"
             and then select the "OK" button. A window titled
             "Install From Disk" will appear.
    Step 3   Specify the path A:\ and select the "OK" button in the
             "Install from Disk" window.
    Step 4   A windows will appear to ask for the "Windows 95 Display
             Driver Disk 2" diskette, Remove the "Windows 95 Display Driver
             Disk 1" diskette and insert "Windows 95 Display Driver Disk 2"
             diskette into floppy drive A. And then specify the path A:\ and
             select the "OK" button.
    Step 5   After all new drivers are installed, a windows will appear to
             ask you to restart Windows 95 now.
    Step 6   Press the "No" button
    Step 7   A message "New Hardware Found PCI card" must be shown on the
             screen.
    Step 8   Select the "Driver from Disk Provided by Hardware Manufacturer"
             and then select the "OK" button. A window titled
             "Install From Disk" will appear.
    Step 9   Specify the path A:\ and select the "OK" button in the
             "Install from Disk" window. (Assume the "Windows 95 Display
             Driver Disk 2" is already in the floppy drive A.)
    Step 10  After this new device is configured, a windows may appear to
             ask you to restart Windows 95 now.
    Step 11  Remove the diskette from floppy drive A and then Press the "Yes"
             button to restart the Windows 95 now. Otherwise, use the normal
             procedure to restart the Windows 95 (In the "Shutdown" sub-menu
              of "Start" menu).


1.2 Updating existing WinFast 3D L2300 Windows 95 drivers

    Step 1   Insert the "Windows 95 Display Driver Disk 1" diskette into
             floppy drive A.
    Step 2   Press the right button of mouse in the Windows 95 wallpaper area.
    Step 3   Select the "Properties" item, a window titled "Display
             Properties" will appear.
    Step 4   Choose the "Settings" tab in the "Display Properties" window.
    Step 5   Select the "Change Display Type" button, a window titled
             "Change Display Type" will appear.
    Step 6   Select the "Change" button in the "Adapter Type" section,
             a window titled "Select Device" will appear.
    Step 7   Select the "Have Disk" button, a window titled
             "Install from Disk" will appear.
    Step 8   Specify the path A:\ and select the "OK" button in the
             "Install from Disk" window.
    Step 9   Select the "OK" button in the "Select Device" window.
    Step 10  A windows will appear to ask for the "Windows 95 Display
             Driver Disk 2" diskette, Remove the "Windows 95 Display Driver
             Disk 1" diskette and insert "Windows 95 Display Driver Disk 2"
             diskette into floppy drive A. And then specify the path A:\ and
             select the "OK" button.
    Step 11  After all new drivers are installed, select the "Close" button
             in the "Change Display Type" window.
    Step 12  Remove the diskette from floppy drive A and then select the
             "Apply" or "Close" button in the "Display Properties" window
    Step 13  A windows will appear to ask you to restart Windows 95 now.
             Restart the Windows 95 now to use the new drivers.

1.3 Trouble Shooting

    If in case you are not able to install the WinFast 3D L2300 Windows 95
    drivers. You can try the following suggested methods to override the
    currently used drivers.

    Method 1: Use another PCI slot which is unused after the Windows 95
              is installed, and the Windows 95 will install the device
              driver(s) for it.

              Step 1   Power off the PC.
              Step 2   Remove the WinFast 3D L2300 board and plug to the
                       another unused PCI slot.
              Step 3   Power on the PC.
              Step 4   During the booting of Windows 95, a message
                       "New hardware Found PCI XGA Compatible Adapter" or
                       "New hardware Found PCI VGA Compatible Adapter" must
                       be shown on the screen. This represents Windows 95
                       can not locate the device driver(s) of WinFast 3D L2300.
                       Follow the section 1.1 to install the drivers of
                       WinFast 3D L2300.

    Method 2: Remove the registry of currently used drivers in the Windows 95
              Safe Mode. (For experienced user)

              Step 1   Reboot the PC.
              Step 2   When your system is rebooted and after the appearance
                       of the "Starting Windows 95" message, press the F5
                       key to enter the Windows 95 Safe Mode.
              Step 3   Select the "Setting" item of "Start" menu.
              Step 4   Select the "Control Panel" item.
              Step 5   Double click on the "System" icon.
              Step 6   Choose the "Device manager" tab.
              Step 7   Remove all the "Display Adapter" device,
                       "PCI XGA Compatible Adapter" and
                       "PCI VGA Compatible Adapter".
                       Especially the display device that you currently
                       used.
              Step 8   Use the normal procedure to restart the Windows 95
                       (In the "Shutdown" sub-menu of "Start" menu).
              Step 9   During the booting of Windows 95, a message
                       "New hardware Found PCI XGA Compatible Adapter" or
                       "New hardware Found PCI VGA Compatible Adapter" must
                       be shown on the screen. This represents Windows 95
                       can not locate the device driver(s) of WinFast 3D L2300.
                       Follow the section 1.1 to install the drivers of
                       WinFast 3D L2300.

    Method 3: Remove the registry and files of currently used drivers
              in the Windows 95 Safe Mode. (For engineer only)

              Step 1   Reboot the PC.
              Step 2   When your system is rebooted and after the appearance
                       of the "Starting Windows 95" message, press the F5
                       key to enter the Windows 95 Safe Mode.
              Step 3   Select the "Setting" item of "Start" menu.
              Step 4   Select the "Control Panel" item.
              Step 5   Double click on the "System" icon.
              Step 6   Choose the "Device manager" tab.
              Step 7   Remove all the "Display Adapter" device,
                       "PCI XGA Compatible Adapter" and
                       "PCI VGA Compatible Adapter".
                       Especially the display device that you currently
                       used.
              Step 8   Delete the OEM*.INF in the Windows INF directory
                       (e.g. del C:\WIN95\INF\OEM*.INF).
                       For the Windows 95 OSR2, you must delete the *.INF
                       in the OTHER sub-directory of Windows INF directory
                       (e.g. del C:\WIN95\INF\OTHER\*.INF).
              Step 9   Delete the *.BIN in the Windows INF directory
                       (e.g. del C:\WIN95\INF\*.BIN).
              Step 10  Delete the currently used display drivers in the
                       Windows SYSTEM directory
                       (e.g. del C:\WIN95\SYSTEM\SUPERS3.*).
                       (e.g. del C:\WIN95\SYSTEM\SUPERVI.*).
              Step 11  Use the "regedit" program to remove all the
                       "Display Device" in the HKEY_LOCAL_MACHINE\Enum\PCI
                        registry.
              Step 12  Use the normal procedure to restart the Windows 95
                       (In the "Shutdown" sub-menu of "Start" menu).
              Step 13  During the booting of Windows 95, a message
                       "New hardware Found PCI XGA Compatible Adapter" or
                       "New hardware Found PCI VGA Compatible Adapter" must
                       be shown on the screen. This represents Windows 95
                       can not locate the device driver(s) of WinFast 3D L2300.
                       Follow the section 1.1 to install the drivers of
                       WinFast 3D L2300.

