=======================================================================

ASUS Display Drivers Readme File for Windows 2000/XP

    Supported Cards and Motherboards:

      ASUS VANTA2000
      ASUS V3800 Series
      ASUS V6600 Series
      ASUS V6800 Series
      ASUS V7100 Series
      ASUS V7700 Series
      ASUS V8200 Series
      ASUS V8170 Series
      ASUS V8420 Series
      ASUS V8440 Series
      ASUS V8460 Series
      ASUS V9180 Series	
      ASUS V9280 Series
      ASUS V9480 Series
      ASUS V9520 Series
      ASUS V9560 Series                        
      ASUS V9900 Series                              
      ASUS V9950 Series 
      ASUS V9980 Series
      ASUS V9570 Series
      ASUS V9400 Series
      ASUS CUA Series

=====================================================================================

Operating systems supported
---------------------------
Microsoft Windows 2000/XP Series

The procedure below describes how to install ASUS display drivers for Windows 2000/XP.



Installing ASUS display drivers for Windows 2000/XP
--------------------------------------------------------------------------------------

Method 1 (ASUS Autorun. Quick installation)
  1. Start Windows.
  2. Put ASUS driver CD into CD-ROM drive.
  3. The AutoPlay function of CD-ROM will work and pop up ASUS Autorun
     window.
  4. Select "Install display driver" option.
  5. Follow the instructions on dialog. Driver will be installed and
     request for restart.
  6. Reboot system and your video adapter is now ready to use.

Method 2 (Run ASUS installation program directly)
  1. Start Windows.
  2. Put ASUS driver CD into CD-ROM drive.
  3. Change to "D:\Win2kXP\ASUS" directory and execute "ANvSETUP.EXE". You also can
     change to "D:\Win2kXP\ANvWest" or "D:\Win2kXP\ANvEast" directory (depending on
     your language) for multi-language support installation and run "setup.exe".
  4. Follow the instructions. Driver will be installed and request for
     restarting.
  5. Reboot system and your video adapter is now ready to use.

Method 3 (Manual installation)
  1. These drivers must be installed by a user with Windows 2000/XP Administrator
     privileges. Please consult your system administrator or Microsoft Windows 2000/XP
     User's Manual for more information on Administrator privileges.
  2. Start Microsoft Windows 2000/XP.
  3. From the Start menu, select Settings.
  4. Select Control Panel.
  5. Select System.
  6. Select Hardware tab.
  7. Select Device Manager.
  8. Select other devices.
  9. Right click the VGA compatible and select Properties.
 10. Select Driver.
 11. Select Update Driver.
 12. Select Next.
 13. Click the box next to "Display a list of the known drivers for this device
     so that I can choose a specific driver" to place a check mark in the box.
     select Next.
 14. Select "Have Disk..."
 15. Windows 2000 will prompt you for the correct path, enter the path of the driver
     such as D:\Win2kXP (assuming your CD-ROM drive is letter D)
 16. A list of video adapters will be displayed. Select the correct card you are using,
     then Click Next.
 17. Select Next.
 18. Select Finish.
 19  Select Close.
 20. Windows 2000/XP will ask if you wish to restart the computer. Select Yes.
     your video adapter is now ready to use.



Uninstall instructions
----------------------
1. These drivers must be uninstalled by a user with Windows 2000/XP Administrator
   privileges.  Please consult your system administrator or Microsoft
   Windows 2000/XP User's Manual for more information on Administrator privileges.
2. Start Microsoft Windows 2000/XP.
3. Click Start control bar option, point to Settings, and click Control Panel.
4. Double-click Add/Remove Programs, click "ASUS Display Drivers", click Add/Remove.
5. Click Yes when asked if you wish to continue.
6. Click OK when asked if you wish to restart the computer.


Important notes
----------------

1. ASUS display cards consume more electrical power so that your
   motherboard must be able to provide enough electrical current in 3.3V
   power to maintain its normal operation.

2. ASUS display cards are recommended to use with Intel 440BX chipset
   for best compatibility.

3. To enable TV-Out function in Windows 2000/XP/NT, just connect the TV connector to the VGA card.
   Don't connect the monitor's 15-pin VGA connector to the VGA card.

4. ASUS Capture driver does not work correctly with ABIT-BP6 MotherBoard.

5. New algorithms for Direct3D VR.

6. To get Vr Picture Viewer worked properly, please install the proper monitor driver
   from Windows or your monitor vendor.

7. ASUS display drivers DO NOT support VR with non-deluxe models. Deluxe models users can enable 
   VR functions from advance page of ASUS control panel.


ASUS Contact Information
------------------------
ASUSTeK COMPUTER INC.
Marketing Info:
Address:   150 Li-Te Road, Peitou, Taipei, Taiwan, ROC
Telephone: +886-2-2894-3447
Fax:       +886-2-2894-3449
Email:     info@asus.com.tw

Technical Support:
Telephone: +886-2-2890-7121
Fax:       +886-2-2895-9254
BBS:       +886-2-2896-4667
Email:     tsd@asus.com.tw
WWW:       http://www.asus.com.tw
News:      news://news2.asus.com.tw
FTP:       ftp://ftp.asus.com.tw/pub/ASUS


ASUS COMPUTER INTERNATIONAL
Marketing Info:
Address:   6737 Mowry Ave, Mowry Business Center Bldg.2, Newark, CA94560, USA
Telephone: +1-510-739-3777
Fax:       +1-510-608-4555
Email:     tmd1@asus.com

Technical Support:
BBS:       +1-510-739-3774
Email:     tsd@asus.com
WWW:       http://www.asus.com
FTP:       ftp://ftp.asus.com.tw/pub/ASUS


ASUS COMPUTER GmbH
Marketing Info:
Address:   Harkort Str.25, 40880 Ratingen, BRD, Germany
Telephone: +49-2102-95990
Fax:       +49-2102-959911
Email:     info@asuscom.de

Technical Support:
BBS:       +49-2102-95990
Email:     tsd@asuscom.de
WWW:       http://www.asuscom.de
FTP:       ftp://ftp.asuscom.de/pub/ASUSCOM
