1. This is ETen Chinese System Display Driver(ETDSPDRV.COM) ver 1.19B01 to
   support SiS VGA Chips. You may update this driver to your ETen Chinese
   System if you have the older version or you may neglect it if you have
   the newer version.

2. How to use?
        a) In default mode (1024x768x16c, 87Hz Interlace), this Display
           Driver will force ET Chinese System to "software scrolling"
           (scrolling with slower speed).
        b) To make use of "hardware scrolling", you must set the Frame
           Rate to non-interlace mode before entering ET Chinese System.
        c) Copy "SVGAUTL.EXE" to <drive>:\<directory>.
        d) Add this line to Autoexec.bat or ET24.bat.
           <drive>:\<directory>\SVGAUTL /F2:60 (60Hz non-interlace)
                        or
           <drive>:\<directory>\SVGAUTL /F2:70 (70Hz non-interlace)
                        or
           <drive>:\<directory>\SVGAUTL /F2:75 (75Hz non-interlace)
          
           Example:
           (1) copy "SVGAUTL.EXE" to C:\SIS
           (2) Add "C:\SIS\SVGAUTL /F2:60" to Autoexec.bat or ET24.bat.

Notes:  1. Some monitors may not support 70Hz and 75Hz non-interlace.
        2. When the stated line was added to ET24.bat, it must be at the
           top of the file.
