
                          Additional Information

                      Sound Galaxy Pro 16 II  v1.10
                     

   This file contains additional information and changes about the
   various software that was not available at printing time.


   CD-ROM Drive Support
   ====================

   The bundled CD-ROM device driver supports only on the following drives:

   Driver           CD-ROM Model
   ------           ------------
   SGIDECD.SYS -   Aztech CDA268-03I / CDA268-03ISE / CDA468-01I /CDA668-01I
                          CDA868-01I


   Installation on Win3.1x Platform
   ================================
   On Windows 3.1x Operating System, choose 'Run' from the 'File' menu. Insert
   the Audio Installation Disk#1 into Drive A: (or Drive B:) and change the path
   to A:\setup (or B:\setup). For more details, you can refer to the Easy Start 
   Manual.


   Installation on Windows 95 Platform
   ===================================
   Start up Windows 95 Operating System. Choose 'Run' from the 'Start' menu and
   insert the Audio Installation Disk#1 into Drive A: (or Drive B:) and change
   the path to 'A:\setup.exe' (or B:\setup.exe) and click OK to install the
   audio drivers as well as the application software.


   Upgrading from Win3.x to Win95 platform
   =======================================
   If you have set up your audio card on a Win3.x platform and want to upgrade
   to Windows 95, remember to remove the audio drivers by doing a deinstallation
   first. For more details, you can refer to the Appendix section in the User's
   Manual.


   Cards with 3D function
   ======================
   If your card has 3D function, after installing SETUP or restarting from
   Windows, you can activate the 3D function by clicking on the '3D' button
   which is located on the audio mixer. 
   For Windows 3.x, the mixer can be found in the program group formed after
   installation.
   For Windows 95, the mixer can be found under the group name formed after
   installation. This is in turn located under 'Programs' in the 'Start' menu.
   The '3D' function can also be activated through the Microsoft Volume Contorl
   Panel.  This can be done by clicking on the default Microsoft 'Speaker' icon
   located at the bottom right corner of the screen.  Choose 'Options' and then
   'Advanced Controls' from menu.  Click on the 'Advanced' button and the 3D
   sound effects can be chosen. 

  

   Latest Windows NT and OS/2 Azt2316/R Audio Drivers   
   ==================================================
   For the latest Windows NT and OS/2 audio drivers, please download from
   our Aztech BBS or at our internet site.


 

        ***********************************************************
        *  In case you encounter any problem with our products,   *
        *  please quote the following model(s) when calling our   *
        *  Technical Support :                                    *
        *                             Oriole 16BB Sound Card      *
        *********************************************************** 



                        -------  The End  ---------
