[Version]
Signature="$Windows95$"
Class=MEDIA		;; needed - this is a wave driver, so gets installed in media
provider=%MFR%

[ClassInstall]
Addreg=Class.AddReg	;; standard media stuff

[Class.AddReg]		;; standard media stuff
HKR,,,,%MediaClassName%
HKR,,Icon,,"-1"
HKR,,Installer,,mmci.dll

[Manufacturer]
%MFR%=PCtel

[PCtel]
%Device1.DeviceDesc%=DEVICE1,  MODEMWAVE\HSP56_MR
 
[DEVICE1]
AddReg=MSSERWAVE.AddReg, DEVICE1.AddReg


[DEVICE1.AddReg]
HKR,Drivers\wave\serwvdrv.drv,Description,,%Device1.DeviceDesc%
HKR,Config,XformModule,  , "umdmxfrm.dll"
HKR,Config,XformID,     1, 04, 00, 00, 00
HKR,Config,WaveDevices,  1, 02, 00		;; normally, have 2 wave devices, line and
						;; handset.  If handset is not supported
						;; only have 1 wave device, so serwvdrv
						;; needs to know this so it only reports
						;; one device.  If this entry is omitted
						;; default is 2

[MSSERWAVE.AddReg]				;; this stuff should never change
HKR,,DevLoader,,mmdevldr.vxd
HKR,Drivers,MIGRATED,,0
HKR,Drivers\wave,,,
HKR,,Driver,,serwave.vxd
HKR,Drivers\wave\serwvdrv.drv,Driver,,serwvdrv.drv
HKR,Drivers,SubClasses,,"wave"

[Strings]
MFR="PCtel, Inc."
Device1.DeviceDesc="PCtel Serial Wave Device"
