; VIAMRAID.INF for winxp
; All rights reserved by  VIA Technologies, Inc. 2003

[Version]
CatalogFile=viamraid.cat
signature="$CHICAGO$"
Class=SCSIAdapter
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}
Provider=%VIA%
DriverVer=05/12/2004, 5.1.2600.310

[DestinationDirs]
DefaultDestDir = 12 ; DIRID_DRIVERS
CopyRAID.NT = 12;

[ControlFlags]

[Manufacturer]
%VIA%=VIA

[VIA]
%PCI\VEN_1106&DEV_3249.DeviceDesc% = viamraid , PCI\VEN_1106&DEV_3249
%PCI\VEN_1106&DEV_3149.DeviceDesc% = viamraid , PCI\VEN_1106&DEV_3149
%PCI\VEN_1106&DEV_3164.DeviceDesc% = viamraid , PCI\VEN_1106&DEV_3164

[VIAMRAID.NT]
CopyFiles=CopyRAID.NT
Reboot

[VIAMRAID.NT.Services]
AddService = viamraid, 2, viamraid_Service_Inst, Miniport_EventLog_Inst


[VIAMRAID_Service_Inst]
ServiceType    = 1      ; SERVICE_KERNEL_DRIVER
StartType      = 0      ; SERVICE_BOOT_START
ErrorControl   = 1      ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\viamraid.sys
LoadOrderGroup = SCSI Miniport
AddReg         = pnp_pci_addreg

[pnp_pci_addreg]
HKR, "Parameters\PnpInterface", "5", 0x00010001, 0x00000001

[Miniport_EventLog_Inst]
AddReg = Miniport_EventLog_AddReg

[Miniport_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,%11%%IOLOGMSGDLL%
HKR,,TypesSupported,%REG_DWORD%,7

[CopyRAID.NT]
viamraid.sys


[SourceDisksFiles]
viamraid.inf = 1
viamraid.sys = 1

[SourceDisksNames]
1 = %DISKNAME1%,,,,
2 = %DISKNAME2%,,,,

[strings]
VIA="VIA Technologies, Inc."
PCI\VEN_1106&DEV_3249.DeviceDesc="VIA VT6421 RAID Controller"
PCI\VEN_1106&DEV_3149.DeviceDesc="VIA SATA RAID Controller"
PCI\VEN_1106&DEV_3164.DeviceDesc="VIA VT6410 RAID Controller"

REG_EXPAND_SZ=0x00020000
REG_DWORD=0x00010001
IOLOGMSGDLL="\IoLogMsg.dll"
DISKNAME1="VIA RAID Driver Diskette"
DISKNAME2="Windows system"