ASUS SmartDoctor v2.74
=====================
1. Search clock information in BIOS then DLL.

ASUS SmartDoctor v2.73
=====================
1. New translucent UI.
2. Add new modle V9560 TD.

ASUS SmartDoctor v2.72
=====================
1. Integrate resources functions.

ASUS SmartDoctor v2.70,  V2.71
=====================
1. Turbo mode for V9560VS

ASUS SmartDoctor v2.69
=====================
1. Change new UI. 
2. Add new modle NV34, NV31 and new feature(FBVDD, NVVDD, AGPBus)
3. Revise Smart Cooling.
4. Revise Calculate mnp.
  
ASUS SmartDoctor v2.68
=====================
1. Add new modle V8170SE
 
ASUS SmartDoctor v2.67 
=====================
1. Add new modle and the latest DLL and SYS files.
2. Different method in getting clock information.
3. Modify "Setup" properly page and FanCtl function.

ASUS SmartDoctor v2.66 beta
=====================
1. Fix AGP3.0 bug in SIS chipset.

ASUS SmartDoctor v2.64
=====================
1. Add new card series(V9280VS).

ASUS SmartDoctor v2.63
=====================
1. Add new card series(V9280).

ASUS SmartDoctor v2.62
=====================
1. Modify the method to adjust clk(level definition). 

ASUS SmartDoctor v2.61
=====================
1. Add a NEW feature: Smart Cooling
   Provide five levels { Off, Low, Median, High, Highest} of Fan-Control.
   Just support V9180 SUITE(with GPIO fan control) now. 
2. Skin shows the level of Fan speed just according to the fan voltage you applied.   
ASUS SmartDoctor v2.51
=====================
1. Add DeviceID for V9280.

ASUS SmartDoctor v2.50
=====================
2002.09.09
----------
1. Replace the kernal mode driver.
   Replace ANVMI.vxd and ANVMI.sys by EIO.vxd and EIO.sys.
   (I2C, AGP mode, Clocking).
2. Add Tweak funaction take place of "Dynamic over clcoking" and 
   "Enable overheat protection". Tweak utility overclock manually.
3. Revise SmartDoctor2's help.
4. Add new skins.
4. InstallShield revise. Detect monitor ic and show different feature to user.
   -- have monitor ic: SmartDoctor feature.
   -- Don't have monitor ic: Tweak feature.
5. If Smartdoctor2 can't work properly, please turn off anti-virus software
   (it's because *.js file).
6. If you want to control core clock from skin, please check the "Run and kepp resident" 
   and uncheck "Enable dynamic graphic cooling".
7. The clock values display on panel maybe slightly different from previous 
   settings. The reason is precision limit. 

ASUS SmartDoctor v2.0
=====================
2002.04.02
----------
1. Add SmartDoctor2's help.
2. Add Voltage error bound for checking VDDQ voltage & AGP Bus 3.3 voltage.
3. Support V8440 Ultra Deluxe Model.

2002.03.14
----------
1. SmartDoctor2 support Win2K/WinXP/Win9X on V8460 Deluxe Model.
2. Only support English version now.




        

